{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-E / ARXC-E"]
[]
[]
[]
[]
["","","","","ATXC20EV1B / ARXC20EV1B","ATXC25EV1B / ARXC25EV1B","ATXC35EV1B / ARXC35EV1B","ATXC50EV1B / ARXC50EV1B","ATXC60EV1B / ARXC60EV1B","ATXC71EV1B / ARXC71EV1B"]
["Unità esterna","","","","ARXC20EV1B","ARXC25EV1B","ARXC35EV1B","ARXC50EV1B","ARXC60EV1B","ARXC71EV1B"]
["Capacità di Raffrescamento","Min.","","kW","1.3","1.3","1.3","1.37","1.8","2.3"]
["","Max.","","kW","3.0","3.0","4.0","6.2","7.0","7.3"]
["Capacità di riscaldamento","Min.","","kW","1.3","1.3","1.3","1.36","1.48","2.3"]
["","Max.","","kW","4.0","4.0","4.8","6.6","8.0","9.0"]
["Efficienza nominale","EER","","","3.33","3.30","3.30","3.25","3.25","2.95"]
["","COP","","","3.73","3.76","3.72","3.71","3.71","3.21"]
["","Classe energetica","Raffreddamento","","A","A","A","A","A","C"]
["","","Riscaldamento","","A","A","A","A","A","C"]
["Raffrescamento ambienti","Classe di efficienza energetica","","","A++","A++","A++","A++","A++","A"]
["","Capacità","Pdesign","kW","2.1","2.6","3.4","5.1","6.2","7.0"]
["","SEER","","","6.8","6.7","6.8","6.4","6.4","5.3"]
["","Consumi energetici annuali","","kWh/a","107","134","177","278","341","464"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Classe di efficienza energetica","","","A+","A+","A+","A+","A+","A"]
["","Capacità","Pdesign","kW","1.9","2.2","2.2","3.9","4.1","6.4"]
["","SCOP/A","","","4.4","4.4","4.3","4.4","4.2","3.8"]
["","Pdh Capacità di riscaldamento a -10°","","kW","1.4","1.6","1.7","3.0","3.5","5.4"]
["","Consumi energetici annuali","","kWh/a","597","708","737","1,249","1,371","2,332"]