{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF25A5V1B","ATXF35A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","40","","","42","44","45"]
["","","","Medio","dBA","34","","","38","40","41"]
["","","","Funzionamento silenzioso","dBA","21","","","30","32","33"]
["","","","Bassa","dBA","28","","","33","35","36"]
["","Raffrescamento","","Medio","dBA","33","","","39","41","42"]
["","","","Funzionamento silenzioso","dBA","20","","","31","33","34"]
["","","","Bassa","dBA","26","","","34","36","37"]
["","","","Alta","dBA","40","","","43","45","46"]
["Accessori standard","Batterie a secco AAA","","","","2","","","2","2","2"]
["","Manuale di installazione","","","","1","","","1","1","1"]
["","Manuale d’uso","","","","1","","","1","1","1"]
["","Telecomando a raggi infrarossi","","","","1","","","1","1","1"]
["","Supporto del telecomando","","","","1","","","1","1","1"]
["","Piastra di montaggio","","","","1","","","1","1","1"]
["","Viti di fissaggio unità interna","","","","2","","","2","2","2"]
["Sistemi di controllo","Telecomando con cavo","","","","BRC944B2, BRC073A1","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","","","ARC470A1","ARC470A1","ARC470A1"]
["Collegamenti tubazioni","Liquido","","DE","mm","6.35","","","6.35","6.35","6.35"]
["","Gas","","DE","mm","9.50","","","12.7","12.7","12.7"]
["","Scarico","","","","18","","","18","18","18"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.019","","","0.029","0.032","0.032"]
["","Riscaldamento","","Nom.","kW","0.020","","","0.032","0.035","0.035"]
["Livello potenza sonora","Raffrescamento","","","dBA","55","","","59","60","62"]
["","Riscaldamento","","","dBA","55","","","61","62","62"]
["Dimensioni","Unità","","Larghezza","mm","770","","","990","990","990"]
["","","","Profondità","mm","225","","","263","263","263"]
["","","","Altezza","mm","286","","","295","295","295"]
["Rivestimento","Colore","","","","Bianco","","","Bianco","Bianco","Bianco"]
["Peso","Unità","","","kg","8.50","","","13.5","13.5","13.5"]
["Ventola","Portata d'aria","Riscaldamento","Alta","m³/min","10.3","","","17.3","17.9","17.9"]
["","","","Bassa","m³/min","6.7","","","12.2","12.8","12.8"]
["","","","Medio","m³/min","8.6","","","14.8","15.8","15.8"]
["","","","Funzionamento silenzioso","m³/min","5.3","","","10.7","11.3","11.3"]
["","","Raffrescamento","Bassa","m³/min","6.1","","","11.9","12.2","12.2"]
["","","","Medio","m³/min","8.1","","","14.4","14.8","14.8"]
["","","","Alta","m³/min","10.1","","","16.8","17.3","17.3"]
["","","","Funzionamento silenzioso","m³/min","4.4","","","10.5","10.7","10.7"]
["Power supply","Fase","","","","1~","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","","","50","50","50"]
["","Nome","","","","","","","V1","V1","V1"]
["","Tensione","","","V","220-240","","","220-240","220-240","220-240"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","0.019","0.032"]
["","Riscaldamento","","Nom.","kW","","0.02","0.032"]
["Rivestimento","Colore","","","","","Bianco","Bianco"]
["Dimensioni","Unità","","Altezza","mm","","286","286"]
["","","","Larghezza","mm","","770","770"]
["","","","Profondità","mm","","225","225"]
["Peso","Unità","","","kg","","8.5","9"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","10.1","11.5"]
["","","","Medio","m³/min","","8.1","8.3"]
["","","","Bassa","m³/min","","6.1","6.3"]
["","","","Funzionamento silenzioso","m³/min","","4.4","4.5"]
["","","Riscaldamento","Alta","m³/min","","10.3","11.5"]
["","","","Medio","m³/min","","8.6","9"]
["","","","Bassa","m³/min","","6.7","7"]
["","","","Funzionamento silenzioso","m³/min","","5.3","5.3"]
["Potenza sonora","Raffrescamento","","","dBA","","55","58"]
["","Riscaldamento","","","dBA","","55","58"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","40","43"]
["Pressione sonora","Raffrescamento","","Medio","dBA","","33","34"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","","26","27"]
["","","","Funzionamento silenzioso","dBA","","20","20"]
["","Riscaldamento","","Alta","dBA","","40","40"]
["Pressione sonora","Riscaldamento","","Medio","dBA","","34","35"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","","28","29"]
["","","","Funzionamento silenzioso","dBA","","21","21"]
["Attacchi tubazioni","Liquido","","DE","mm","","6.35","6.35"]
["","Gas","","DE","mm","","9.5","9.5"]
["","Scarico","","","","","18","18"]
["Sistemi di controllo","Telecomando infrarossi","","","","","ARC470A1","ARC470A1"]
["","Telecomando con cavo","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Accessori standard","Installation manual","","","","","1","1"]
["","AAA dry-cell batteries","","","","","2","2"]
["","Operation manual","","","","","1","1"]
["","Indoor unit fixing screws","","","","","2","2"]
["","Infrared remote control","","","","","1","1"]
["","Mounting plate","","","","","1","1"]
["","Remote control holder","","","","","1","1"]
["Alimentazione","Fase","","","","","1~","1~"]
["","Frequenza","","","Hz","","50","50"]
["","Tensione","","","V","","220-240","220-240"]