{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXL-JV"]
[]
[]
[]
[]
["","","","","ATXL25J2V1B","ATXL35J2V1B"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","41","41"]
["","","Funzionamento silenzioso","dBA","26","26"]
["","","Bassa","dBA","29","29"]
["","Raffrescamento","Funzionamento silenzioso","dBA","23","23"]
["","","Bassa","dBA","27","27"]
["","","Alta","dBA","41","41"]
["","","Nom.","dBA","35","35"]
["","Raffrescamento","Nom.","dBA","34","34"]
["Accessori standard","Manuale di installazione","","","1","1"]
["","Manuale d’uso","","","1","1"]
["","Telecomando a raggi infrarossi","","","1","1"]
["","Batterie","","","2","2"]
["","Supporto del telecomando","","","1","1"]
["","Piastra di montaggio","","","1","1"]
["","Filtro purificatore d'aria a base di apatite e titanio","","","2","2"]
["","Viti di fissaggio unità interna","","","2","2"]
["Sistemi di controllo","Infrared remote control","","","ARC433A87","ARC433A87"]
["Piping connections","Liquido","DE","mm","6.35","6.35"]
["","Gas","DE","mm","9.5","9.5"]
["","Scarico","","","18","18"]
["Potenza assorbita","Raffrescamento","Nom.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["","Riscaldamento","Nom.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["Livello potenza sonora","Raffrescamento","","dBA","57","57"]
["","Riscaldamento","","dBA","57","57"]
["Dimensioni","Unità","Larghezza","mm","770","770"]
["","","Profondità","mm","198","198"]
["","","Altezza","mm","283","283"]
["Rivestimento","Colour","","","Bianco","Bianco"]
["Peso","Unità","","kg","8","8"]
["Power supply","Phase","","","1~","1~"]
["","Frequenza","","Hz","50","50"]
["","Nome","","","V1","V1"]
["","Tensione","","V","220-240","220-240"]
["Note","","","","(1) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare.","(1) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]