{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B","ATXP25N5V1B","ATXP35N5V1B"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.019","0.02","0.032"]
["","Riscaldamento","","Nom.","kW","0.023","0.023","0.032"]
["Rivestimento","Colore","","","","Bianco","Bianco","Bianco"]
["Dimensioni","Unità","","Altezza","mm","286","286","286"]
["","","","Larghezza","mm","770","770","770"]
["","","","Profondità","mm","225","225","225"]
["Peso","Unità","","","kg","8.5","8.5","9"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","9.5","9.7","11.5"]
["","","","Medio","m³/min","7.4","7.7","8.3"]
["","","","Bassa","m³/min","5.6","5.8","6.3"]
["","","","Funzionamento silenzioso","m³/min","4.2","4.2","4.5"]
["","","Riscaldamento","Alta","m³/min","10.4","10.4","11.5"]
["","","","Medio","m³/min","8.1","8.1","9"]
["","","","Bassa","m³/min","6.2","6.4","7"]
["","","","Funzionamento silenzioso","m³/min","5.2","5.2","5.3"]
["Potenza sonora","Raffrescamento","","","dBA","55","55","58"]
["","Riscaldamento","","","dBA","55","55","58"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","39","40","43"]
["Pressione sonora","Raffrescamento","","Medio","dBA","33","33","34"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","25","26","27"]
["","","","Funzionamento silenzioso","dBA","19","19","20"]
["","Riscaldamento","","Alta","dBA","39","40","40"]
["Pressione sonora","Riscaldamento","","Medio","dBA","34","34","35"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","28","28","29"]
["","","","Funzionamento silenzioso","dBA","21","21","21"]
["Attacchi tubazioni","Liquido","","DE","mm","6","6","6"]
["","Gas","","DE","mm","9.5","9.5","9.5"]
["","Scarico","","","","18","18","18"]
["Sistemi di controllo","Telecomando infrarossi","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Telecomando con cavo","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Accessori standard","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1"]
["","Silver particle filter","","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Alimentazione","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240"]