{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53A"]
[]
[]
[]
[]
["","","","","BRC1E53A7"]
["Rivestimento","Colore","","","Bianco frizzante"]
["","Coperchio pulsantiera","","","No"]
["","LED di funzionamento","Colore","","Verde"]
["Dimensioni","Unità","Altezza","mm","120"]
["","","Larghezza","mm","120"]
["","","Profondità","mm","19"]
["","Unità imballata","Altezza","mm","55"]
["","","Larghezza","mm","160"]
["","","Profondità","mm","150"]
["Peso","Unità","","kg","0.200"]
["","Unità imballata","","kg","0.415"]
["Guarnizione","Materiale","","","Cartone_"]
["","Peso","","kg","0.05"]
["LCD","Tipo","","","Full dot (160 x 255)"]
["","Dimensioni","Altezza","mm","43.2"]
["","","Larghezza","mm","68.85"]
["","Retroilluminazione","Colore","","Bianco"]
["Temperatura esterna","Funzionamento","Min.","°C","-10"]
["","","Max.","°C","50"]
["","Magazzinamento","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Umidità relativa <","","%","95"]
["Collegamenti elettrici","Lunghezza cablaggio","Max.","m","500"]
["Backup per interruzione di corrente","","","","Sì (l'orologio continua a funzionare per un periodo non superiore alle 48 ore)"]