{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW (Archived)"]
["Rivestimento","Colore","","","Bianco"]
["","Coperchio pulsantiera","","","No"]
["","LED di funzionamento","Colore","","Indicatore di stato blu"]
["Dimensioni","Unità","Altezza","mm","85"]
["","","Larghezza","mm","85"]
["","","Profondità","mm","25"]
["","Unità imballata","Altezza","mm","50"]
["","","Larghezza","mm","217"]
["","","Profondità","mm","161"]
["Peso","Unità","","kg","0.110"]
["","Unità imballata","","kg","0.317"]
["Imballaggio","Materiale","","","Cartone"]
["Guarnizione","Peso","","kg","0.0850"]
["LCD","Tipo","","","100 x 150 punti"]
["","Dimensioni","Altezza","mm","40.7"]
["","","Larghezza","mm","28.0"]
["","Retroilluminazione","Colore","","Bianco"]
["Temperatura esterna","Funzionamento","Min.","°C","-10"]
["","","Max.","°C","52"]
["","Magazzinamento","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Temperatura esterna-=-Umidità relativa <-=-%","","%","95"]
["Sistemi di comando","Controllo classe di temperatura","","","VI"]
["","Contributo all'efficienza stagionale riscaldamento ambienti","","%","4.0"]
["Collegamenti elettrici","Lunghezza cablaggio","Max.","m","500"]