{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A5A"]
[]
[]
[]
[]
["","","","","","D2C18ND024A5AA","D2C20ND028A5AA","D2C24ND035A5AA"]
["Gas","Consumi (G20)","","Min","m³/h","0.31","0.51","0.51"]
["","","","Max","m³/h","1.80","2.04","2.45"]
["","Consumi (G25)","","Min","m³/h","0.36","0.59","0.59"]
["","","","Max","m³/h","2.09","2.35","2.85"]
["","Consumi (G31)","","Min","m³/h","0.12","0.20","0.20"]
["","","","Max","m³/h","0.69","0.98","1.19"]
["","Classe NOx","","","","6","6","6"]
["","Livelli di NOx (G20)","","","mg/kWh","18","31","32"]
["Riscaldamento centralizzato","Assorbimento di calore Qn (valore calorifico netto)","Nom.","Min","kW","2.9","4.8","4.8"]
["","","","Max","kW","16.9","19.2","23.5"]
["","Assorbimento di calore Qn (valore calorifico lordo)","Nom.","Min","kW","3.2","5.3","5.3"]
["","","","Max","kW","18.8","21.3","26.1"]
["","Pn in uscita a 80/60°C","","Min","kW","2.8","4.6","4.6"]
["","","","Nom.","kW","16.4","18.8","22.9"]
["","Pn in uscita a 50/30°C","","Riscaldamento centralizzato-=-Pn in uscita a 50/30°C-=-Min-=-kW","kW","3.1","5.2","5.2"]
["","","","Nom.","kW","18.0","20.0","24.0"]
["","Potenza a 37/30°C","","Nom.","kW","5.5","6.3","7.7"]
["","Temperatura acqua","","Max","°C","100","100","100"]
["Acqua calda sanitaria","Assorbimento di calore (valore calorifico netto) Qnw","Nom.","Min","kW","2.9","4.8","4.8"]
["","","","Max","kW","25.3","29.5","34.0"]
["","Assorbimento di calore (valore calorifico lordo) Qnw","Nom.","Min","kW","3.2","5.3","5.3"]
["","","","Max","kW","27.7","32.7","37.7"]
["","Classe di comfort (EN13203)","","","","***","***","***"]
["","Temperatura","","Max","°C","70","70","70"]
["Aria di immissione","Collegamento","","","mm","100","100","100"]
["","Concentrico","","","","Sì","Sì","Sì"]
["Gas combustibile","Temperatura","","Max","°C","77","76","82"]
["","Collegamento","","","mm","60","60","60"]
["","Portata (G20)","","Max","kg/ora","38.7","44.5","55.7"]
["","Portata (G31)","","Max","kg/ora","36.0","43.3","54.8"]
["Rivestimento","Colore","","","","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)"]
["","Materiale","","","","Lamiera d'acciaio zincata verniciata a polvere","Lamiera d'acciaio zincata verniciata a polvere","Lamiera d'acciaio zincata verniciata a polvere"]
["Dimensioni","Unità","Altezza","Struttura","mm","590","695","695"]
["","","","Larghezza","mm","400","440","440"]
["","","","Profondità","mm","256","295","295"]
["Peso","Unità","","Vuoto","kg","27","37","37"]
["Riscaldamento acqua calda sanitaria","Generale","","Riscaldamento acqua calda sanitaria-=-Generale-=-Profilo di carico dichiarato","","XL","XL","XL"]
["","","","Classe di efficienza energetica riscaldamento acqua","","A","A","A"]
["Riscaldamento ambienti","Generale","","Classe efficienza stagionale riscaldamento ambienti","","A","A","A"]