{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":15,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2TND-A4A"]
[]
[]
[]
[]
["","","","","","D2TND012A4AA","D2TND012A4AB","D2TND018A4AA","D2TND018A4AB","D2TND024A4AA","D2TND024A4AB","D2TND035A4AB","D2TND035A4AA","D2TND028A4AA","D2TND028A4AB"]
["Gas","Consumi (G20)","","Min","m³/h","0.31","0.31","0.31","0.31","0.31","0.31","0.511","0.511","0.511","0.511"]
["","","","Max","m³/h","1.18","1.18","1.80","1.8","2.48","2.48","3.63","3.63","2.89","2.89"]
["","Consumi (G25)","","Min","m³/h","0.36","0.36","0.36","0.36","0.36","0.36","0.59","0.59","0.59","0.59"]
["","","","Max","m³/h","1.38","1.38","2.09","2.09","2.89","2.89","4.19","4.19","3.32","3.32"]
["","Consumi (G31)","","Min","m³/h","0.12","0.12","0.12","0.12","0.12","0.12","0.2","0.2","0.2","0.2"]
["","","","Max","m³/h","0.46","0.46","0.69","0.69","0.96","0.96","1.38","1.38","1.1","1.1"]
["","Classe NOx","","","","6","6","6","6","6","6","6","6","6","6"]
["","Livelli di NOx (G20)","","","mg/kWh","10","10","18","18","22","22","35.5","35.5","36.3","36"]
["Riscaldamento centralizzato","Assorbimento di calore Qn (valore calorifico netto)","Nom.","Min","kW","2.9","2.9","2.9","2.9","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max","kW","11.2","11.1","17.0","16.9","23.5","23.5","34","34","27","27"]
["","Assorbimento di calore Qn (valore calorifico lordo)","Nom.","Min","kW","3.2","3.2","3.2","3.2","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max","kW","12.4","12.3","18.9","18.8","26.1","26.1","37.8","37.8","30","30"]
["","Pn in uscita a 80/60°C","","Min","kW","2.8","2.8","2.8","2.8","2.8","2.8","4.6","4.6","4.6","4.6"]
["","","","Nom.","kW","10.9","10.9","16.6","16.6","22.8","22.8","33.2","33.2","26.3","26.3"]
["","Pn in uscita a 50/30°C","","Riscaldamento centralizzato-=-Pn in uscita a 50/30°C-=-Min-=-kW","kW","3.1","3.1","3.1","3.1","3.1","3.1","5.2","5.2","5.2","5.2"]
["","","","Nom.","kW","12.0","12","18.0","18","24.0","24","35","35","28.2","28.2"]
["","Potenza a 37/30°C","","Nom.","kW","3.7","3.7","5.6","5.5","7.6","7.6","11.1","11.1","8.8","8.8"]
["","Temperatura acqua","","Max","°C","100","100","100","100","100","100","100","100","100","100"]
["","Efficienza","","Valore calorifico netto","%","98.6","98.6","98.2","98.2","97.9","97.9"]
["","","","Valore calorifico lordo","%","87.8","87.8","87.4","87.4","87.3","87.3"]
["Acqua calda sanitaria","Assorbimento di calore (valore calorifico netto) Qnw","Nom.","Min","kW","2.9","2.9","2.9","2.9","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max","kW","11.2","11.1","17.0","16.9","23.5","25.3","34","34","29.5","29.5"]
["","Assorbimento di calore (valore calorifico lordo) Qnw","Nom.","Min","kW","3.2","3.2","3.2","3.2","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max","kW","12.4","12.3","18.1","18.1","26.1","26.1","37.7","37.7","32.7","32.7"]
["","Temperatura","","Max","°C","60","60","60","60","60","60","60","60","60","60"]
["Dispersione termica","Caldaia di riserva Ps","","","kW","0.057","0.057","0.057","0.057","0.057","0.057","0.065","0.0650","0.0650","0.065"]
["Aria di immissione","Collegamento","","","mm","100","100","100","100","100","100","100","100","100","100"]
["","Concentrico","","","","Sì","Sì","Sì","Sì","Sì","Sì","Sì","Sì","Sì","Sì"]
["Gas combustibile","Temperatura","","Max","°C","90","90","90","90","90","90","81.7","81.7","76.4","76.4"]
["","Collegamento","","","mm","60","60","60","60","60","60","60","60","60","60"]
["","Portata (G20)","","Max","kg/ora","38.7","38.7","38.7","38.7","38.7","38.7","55.7","55.7","44.5","55.7"]
["","Portata (G25)","","Max","kg/ora","","","","","","","49.6","49.6","39.3","39.3"]
["","Portata (G31)","","Max","kg/ora","36.0","36","36.0","36","36.0","36","54.7","54.7","43.3","43.3"]
["Rivestimento","Colore","","","","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)"]
["","Materiale","","","","Lamiera","Lamiera","Lamiera","Lamiera","Lamiera","Lamiera","Lamiera d'acciaio zincata verniciata a polvere","Lamiera d'acciaio zincata verniciata a polvere","Lamiera d'acciaio zincata verniciata a polvere","Lamiera d'acciaio zincata verniciata a polvere"]
["Dimensioni","Unità","Altezza","Struttura","mm","590","590","590","590","590","590","690","690","690","690"]
["","","","Larghezza","mm","400","400","400","400","400","400","440","440","440","440"]
["","","","Profondità","mm","256","256","256","256","256","256","295","295","295","295"]
["Peso","Unità","","Vuoto","kg","27","27","27","27","27","27","1","35.5","35.5","1"]
["","","","Piena","kg","27","27.0","27","27.0","27","27.0","","37.5","37.5"]
["","Caldaia","","Vuoto","kg","26.5","26.5","26.5","26.5","26.5","26.5"]
["Riscaldamento ambienti","Generale","","Classe efficienza stagionale riscaldamento ambienti","","A","A","A","A","A","A","A","A","A","A"]