{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Potenza assorbita","kW","","","","0.015"]
["Massimo numero di unità interne collegabili","","","","","32"]
["Massimo numero di unità esterne collegabili @","","","","","7"]
["Dimensioni","Unità","","Altezza","mm","136"]
["","","","Larghezza","mm","384"]
["","","","Profondità","mm","92"]
["Comunicazione","DIII-NET","","Quantità","","1"]
["","","","Nota","","DIII-NET (F1F2)"]
["","Ethernet","","Quantità","","1"]
["","Morsetto di ingresso","Digitale","Quantità","","4"]
["Temperatura esterna","Funzionamento","","Min.","°C","-10"]
["","","","Max.","°C","50"]
["","Magazzinamento","","Min.","°C","-20"]
["","","","Max.","°C","60"]
["","Temperatura esterna-=-Umidità relativa <-=-%","","","%","85"]
["Alimentazione","Frequenza","","","Hz","50/60"]
["","Tensione","","","V","110-240 AC"]
["Note","","","","","(1) - Comprende la potenza assorbita dell'alimentatore WAGO, il modulo CPU e il modulo I/O"]
["","","","","","(2) - Le dimensioni comprendono l'alimentatore WAGO, il modulo CPU, il modulo I/O e lo spazio necessario tra le varie parti"]
["","","","","","(3) - Le dimensioni dello schermo opzionale sono: altezza: 209 mm, larghezza: 123 mm, profondità: 8,5 mm"]