{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Livello pressione sonora","Nom.","","","dBA","32.0 (6)"]
["Refrigerante","GWP","","","","2,090"]
["","Carica","","","kg","1.80"]
["","Tipo","","","","R-410A"]
["Campo di funzionamento","Ingombro","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Heating","Lato acqua","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Lato salamoia","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Acqua calda sanitaria","Lato acqua","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Potenza assorbita","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Livello potenza sonora","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Dimensioni","Unità","","Larghezza","mm","600"]
["","","","Profondità","mm","728"]
["","","","Altezza","mm","1,730"]
["Rivestimento","Materiale","","","","Piastra di lamiera rivestita"]
["","Colour","","","","Bianco"]
["Serbatoio","Volume acqua","","","l","180"]
["","Protezione contro la corrosione","","","","Anodo"]
["","Isolante","","Perdita di calore","kWh/24h","1.36 (4)"]
["Peso","Unità","","","kg","210"]
["Risc. amb.","Uscita acqua cond. clim. medie 35°C","Generale","ηs (Efficienza stagionale Risc. amb.)","%","194"]
["","","","Classe efficienza stagionale Risc. amb.","","A+++"]
["","","","SCOP","","5.06"]
["","Uscita acqua cond. clim. medie 55°C","Generale","Seasonal space heating eff. class","","A++"]
["","","","ηs (Efficienza stagionale Risc. amb.)","%","139"]
["","","","SCOP","","3.68"]
["Capacità di riscaldamento","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Fase","","","","3~"]
["","Nome","","","","9W"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","400"]
["Corrente","Fusibili consigliati","","","A","25"]
["Note","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45°C (DT=5°C)"]
["","","","","","(3) - con il 40% di glicole propilenico"]
["","","","","","(4) - Perdita di calore conforme allo standard EN12897"]
["","","","","","(5) - Comprese tubazioni + scambiatore di calore a piastre + riscaldatore di riserva, escluso vaso di espansione"]
["","","","","","(6) - Il livello di pressione sonora viene misurato mediante microfono posto ad 1m di distanza dall’unità. È un valore relativo e dipende dalla distanza e dall'ambiente acustico."]
["","","","","","(7) - Con la pompa di calore"]
["","","","","","(8) - Con pompa di calore + riscaldatore elettrico di riserva"]
["","","","","","(9) - Con il riscaldatore elettrico di riserva"]