{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-E"]
[]
[]
[]
[]
["","","","","","EHSX04P30EG","EHSX04P50EG","EHSX08P30EG","EHSX08P50EG","EHSX04P30EF (Archived)","EHSX04P50EF (Archived)","EHSX08P30EF (Archived)","EHSX08P50EF (Archived)"]
["Rivestimento","Colore","","","","Bianco opaco (RAL9016) / Nero opaco (RAL9017)","Bianco opaco (RAL9016) / Nero opaco (RAL9017)","Bianco opaco (RAL9016) / Nero opaco (RAL9017)","Bianco opaco (RAL9016) / Nero opaco (RAL9017)","Bianco opaco (RAL9016) / Nero opaco (RAL9017)","Bianco opaco (RAL9016) / Nero opaco (RAL9017)","Bianco opaco (RAL9016) / Nero opaco (RAL9017)","Bianco opaco (RAL9016) / Nero opaco (RAL9017)"]
["","Materiale","","","","Polipropilene resistente agli urti","Polipropilene resistente agli urti","Polipropilene resistente agli urti","Polipropilene resistente agli urti","Polipropilene resistente agli urti","Polipropilene resistente agli urti","Polipropilene resistente agli urti","Polipropilene resistente agli urti"]
["Dimensioni","Unità","","Altezza","mm","1891","1910","1891","1910","1892","1905","1892","1905"]
["","","","Larghezza","mm","594","792","594","792","594","792","594","792"]
["","","","Profondità","mm","644","817","644","817","644","812","644","812"]
["Peso","Unità","","","kg","77.0","97.0","77.0","97.0","77","107","77","107"]
["PED","Categoria","","","","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0","675","675","675","675"]
["","Carica","","","kg","1.50","1.50","1.50","1.50","1.5","1.5","1.5","1.5"]
["Livello potenza sonora","Nom.","","","dBA","39","39","39","39","39","39","39","39"]
["Campo di funzionamento","Riscaldamento","Lato acqua","Min.","°C","18","18","18","18","18","18","18","18"]
["","","","Max.","°C","65","65","65","65","65","65","65","65"]
["","Raffrescamento","T. esterna","Min.","°CBS","10","10","10","10","10","10","10","10"]
["","","Lato acqua","Min.","°C","5","5","5","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22","22","22","22"]
["Alimentazione","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50","50","50","50","50","50"]
["","Tensione","","","V","230","230","230","230","230","230","230","230"]
["Note","","","","","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897","(1) - Perdita di calore conforme allo standard EN12897"]