{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","EHY2KOMB28AA","EHY2KOMB32AA"]
["Acqua calda sanitaria","Assorbimento di calore (valore calorifico lordo) Qnw","Nom.","Max","kW","32.3","36.3"]
["","","","Min","kW","7.9","8.4"]
["","Classe di comfort (EN13203)","","","","XL","XL"]
["","Temperatura","","Max","°C","65","65"]
["","Assorbimento di calore (valore calorifico netto) Qnw","Nom.","Min","kW","7.1","7.6"]
["","","","Max","kW","29.1","32.7"]
["Gas combustibile","Portata (G25)","","Max","kg/ora","48.6","54.4"]
["","Portata (G20)","","Max","kg/ora","48.6","54.4"]
["","Portata (G31)","","Max","kg/ora","47.9","53.6"]
["","Temperatura","","Max","°C","70","70"]
["Aria di immissione","Concentrico","","","","60/100","60/100"]
["Riscaldamento acqua calda sanitaria","Generale","","Classe di efficienza energetica riscaldamento acqua","","A","A"]
["","","","Profilo di carico dichiarato","","XL","XL"]
["Dimensioni","Unità","Altezza","Struttura","mm","650","710"]
["Rivestimento","Materiale","","","","Piastra di lamiera rivestita","Piastra di lamiera rivestita"]
["","Colore","","","","RAL9010","RAL9010"]
["Risc. amb.","Generale","","ηs (Efficienza stagionale riscaldamento ambienti)","%","92","93"]
["","","","Classe efficienza stagionale riscaldamento ambienti","","A","A"]
["Riscaldamento centralizzato","Assorbimento di calore Qn (valore calorifico lordo)","Nom.","Min","kW","7.9","8.4"]
["","","","Max","kW","26.3","30.0"]
["","Temperatura acqua","","Max","°C","90","90"]
["","Potenza a 37/30°C","","Nom.","kW","7.7","8.2"]
["","Pn in uscita a 80/60°C","","Min","kW","7.1","7.4"]
["","","","Nom.","kW","23.1","26.6"]
["","Assorbimento di calore Qn (valore calorifico netto)","Nom.","Min","kW","7.1","7.6"]
["","","","Max","kW","23.7","27.0"]
["","Pn in uscita a 50/30°C","","Min","kW","7.7","8.2"]
["","","","Nom.","kW","25.4","28.9"]
["Gas","Livelli di NOx (G20)","","","mg/kWh","27","36"]
["","Consumi (G25)","","Min","m³/ora","0.84","0.89"]
["","","","Max","m³/ora","3.46","3.92"]
["","Classe NOx","","","","6","6"]
["","Attacco","","Diametro","mm","15","15"]
["","Consumi (G20)","","Max","m³/ora","3.02","3.39"]
["","","","Min","m³/ora","0.74","0.79"]
["","Consumi (G31)","","Min","m³/ora","0.28","0.30"]
["","","","Max","m³/ora","1.15","1.29"]