{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AAV3 / EVLQ08CAV3"]
["Riscaldamento acqua calda sanitaria","Generale","","Profilo di carico dichiarato","","XL"]
["","Condizioni climatiche medie","","Classe di efficienza energetica riscaldamento acqua","","A"]
["COP","","","","","4.45 (3), 3.42 (4)"]
["Risc. amb.","Uscita acqua cond. clim. medie 55°C","Generale","Seasonal space heating eff. class","","A++"]
["","","","ηs (Efficienza stagionale Risc. amb.)","%","129"]
["","","","SCOP","","3.29"]
["Capacità di Raffrescamento","Nom.","","","kW","6.86 (4), 5.36 (4)"]
["","Min.","","","kW","2.50 (3), 2.50 (4)"]
["EER","","","","","3.42 (3), 2.29 (4)"]
["Capacità di riscaldamento","Nom.","","","kW","7.40 (3), 6.89 (4)"]
["","Min.","","","kW","1.80 (3), 1.80 (4)"]
["","Max.","","","kW","10.0 (3), 9.53 (4)"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","2.01 (3), 2.34 (4)"]
["","Riscaldamento","","Nom.","kW","1.66 (3), 2.01 (4)"]
["Note","","","","","(1) - Stato: Ta BS/BU 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Stato: Ta BS/BU 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Condizione 1: raffreddamento Ta 35°C - LWE 18°C (DT = 5°C); riscaldamento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Condizione 2: raffreddamento Ta 35°C - LWE 7°C (DT = 5°C); riscaldamento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(5) - T. est. 35°C – LWE 7°C (DT=5°C), caldaia bypassata"]
["","","","","","(6) - T. est. 35°C – LWE 18℃ (DT=5°C), caldaia bypassata"]
["","","","","","(7) - BS/BU 7°C/6°C - LWC 35°C (DT=5°C), bypass caldaia"]
["","","","","","(8) - BS/BU 7°C/6°C - LWC 45°C (DT=5°C), bypass caldaia"]