{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Rivestimento","Colore","","","","Bianco"]
["","Materiale","","","","Piastra di lamiera rivestita"]
["Dimensioni","Unità","","Altezza","mm","902"]
["","","","Larghezza","mm","450"]
["","","","Profondità","mm","164"]
["Peso","Unità","","","kg","31.2"]
["PED","Categoria","","","","Categoria I"]
["Scambiatore di calore lato acqua","Portata acqua","Riscaldamento","Max.","l/min","23.5 (7)"]
["Livello potenza sonora","Nom.","","","dBA","42.0"]
["Campo di funzionamento","Riscaldamento","Lato acqua","Min.","°C","25 (8)"]
["","","","Max.","°C","55 (8)"]
["","Raffrescamento","T. esterna","Min.","°CBS","10 (8)"]
["","","Lato acqua","Min.","°C","5 (8)"]
["","","","Max.","°C","22 (8)"]
["Alimentazione","Nome","","","","V3"]
["","Fase","","","","1~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","230"]
["Collegamenti elettrici","Per collegamento con interfaccia utente","","Quantità","","2"]
["","","","Osservazioni","","Da 0,75 mm² a 1,25 mm² (lunghezza max. 500 m)"]
["Note","","","","","(1) - Solo per unità interna"]
["","","","","","(2) - BS/BU 7°C/6°C - LWC 35°C (DT=5°C), bypass caldaia"]
["","","","","","(3) - BS/BU 7°C/6°C - LWC 45°C (DT=5°C), bypass caldaia"]
["","","","","","(4) - T. est. 35°C – LWE 7°C (DT=5°C), caldaia bypassata"]
["","","","","","(5) - T. est. 35°C – LWE 18℃ (DT=5°C), caldaia bypassata"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Bypass caldaia"]
["","","","","","(8) - Per il campo di funzionamento di *HYHB* e *HYKOMB33AA, vedere gli schemi relativi al campo di funzionamento"]