{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYKOMB-AA3"]
[]
[]
[]
[]
["","","","","","EHYKOMB33AA3"]
["Gas","Attacco","","Diametro","mm","15"]
["","Consumi (G20)","","Min","m³/ora","0.79"]
["","","","Max","m³/ora","3.39"]
["","Consumi (G25)","","Min","m³/ora","0.89"]
["","","","Max","m³/ora","3.92"]
["","Consumi (G31)","","Min","m³/ora","0.30"]
["","","","Max","m³/ora","1.29"]
["","Classe NOx","","","","6"]
["","Livelli di NOx (G20)","","","mg/kWh","36"]
["Riscaldamento centralizzato","Assorbimento di calore Qn (valore calorifico netto)","Nom.","Min","kW","7.6"]
["","","","Max","kW","27.0"]
["","Assorbimento di calore Qn (valore calorifico lordo)","Nom.","Min","kW","8.4"]
["","","","Max","kW","30.0"]
["","Pn in uscita a 80/60°C","","Min","kW","7.5"]
["","","","Nom.","kW","26.6"]
["","Potenza a 37/30°C","","Nom.","kW","8.2"]
["","Temperatura acqua","","Max","°C","90"]
["Acqua calda sanitaria","Assorbimento di calore (valore calorifico netto) Qnw","Nom.","Min","kW","7.6"]
["","","","Max","kW","32.7"]
["","Assorbimento di calore (valore calorifico lordo) Qnw","Nom.","Min","kW","8.4"]
["","","","Max","kW","36.3"]
["","Classe di comfort (EN13203)","","","","XL"]
["","Temperatura","","Max","°C","65"]
["Aria di immissione","Concentrico","","","","No"]
["Gas combustibile","Temperatura","","Max","°C","70"]
["","Collegamento","","","mm","60"]
["","Portata (G20)","","Max","kg/h","54.4"]
["","Portata (G25)","","Max","kg/h","54.4"]
["","Portata (G31)","","Max","kg/h","53.6"]
["Rivestimento","Colore","","","","RAL9010"]
["","Materiale","","","","Piastra di lamiera rivestita"]
["Dimensioni","Unità","Altezza","Struttura","mm","710"]
["","","","Larghezza","mm","450"]
["","","","Profondità","mm","240"]
["Peso","Unità","","Vuoto","kg","36"]
["Riscaldamento acqua calda sanitaria","Generale","","Riscaldamento acqua calda sanitaria-=-Generale-=-Profilo di carico dichiarato","","XL"]
["","","","Classe di efficienza energetica riscaldamento acqua","","A"]
["Riscaldamento ambienti","Generale","","Classe efficienza stagionale riscaldamento ambienti","","A"]