{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSRPS4A"]
[]
[]
[]
[]
["","","","","EKSRPS4A.","EKSRPS4AB"]
["Temperatura non in funzionamento","Max.","","°C","85","85"]
["Dimensioni","Unità","Larghezza","mm","142","142"]
["","","Profondità","mm","230","230"]
["","","Altezza","mm","815","815"]
["Peso","Unità","","kg","6","6.4"]
["Campo di funzionamento","Ambient temperature","Max.","°C","40","40"]
["","","Min.","°C","5","5"]
["Pressione d'esercizio","Max.","","bar","","0"]
["Montaggio","","","","Sul lato del serbatoio","Sul lato del serbatoio"]
["Ingresso alimentazione","","","","Unità interna","Unità interna"]
["Controllo","Tipo","","","Regolatore di temperatura differenziale digitale con display solo testo","Regolatore di temperatura differenziale digitale con display solo testo"]
["","Consumo energetico","","W","2","2"]
["Power supply","Fase","","","1~","1~"]
["","Frequenza","","Hz","50","50"]
["","Tensione","","V","230","230"]