{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK06-10AV3"]
[]
[]
[]
[]
["","","","","","EPSK06ARV3","EPSK08ARV3","EPSK10ARV3"]
["Dimensioni","Unità","","Altezza","mm","1123","1123","1123"]
["","","","Larghezza","mm","1330","1330","1330"]
["","","","Profondità","mm","604","604","604"]
["Peso","Unità","","","kg","174","174","174"]
["Ventilatore","Portata d'aria","Riscaldamento","Alta","m³;/min","75.7","75.7","75.7"]
["","","Raffrescamento","Alta","m³;/min","75.7","75.7","75.7"]
["Campo di funz.","Raffresc.","","Min.","°CBS","10","10","10"]
["","","","Max.","°CBS","43","43","43"]
["Campo di funzionamento","Acqua calda sanitaria","","Min.","°CBS","-28","-28","-28"]
["Campo di funz.","Acqua calda sanitaria","","Max.","°CBS","40","40","40"]
["Livello potenza sonora","Riscaldamento","","Nom.","dBA","45 (1)","45 (1)","47 (1)"]
["","Raffrescamento","","Nom.","dBA","52.2 (2)","53 (2)","53.2 (2)"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","32.6 (1)","32.4 (1)","32.8 (1)"]
["","Raffrescamento","","Nom.","dBA","36.9 (2)","37.2 (2)","37.3 (2)"]
["Refrigerante","Tipo","","","","R-290","R-290","R-290"]
["","GWP","","","","3","3","3"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","0.003","0.003","0.003"]
["","Carica","","","kg","1","1","1"]
["Collegamenti tubazioni","Dislivello","int. - est.","Max.","m","10","10","10"]
["Alimentazione","Nome","","","","V3","V3","V3"]
["","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","230","230","230"]
["Corrente","Fusibili consigliati","","","A","25","25","25"]
["Note","","","","","(1) - Misurata con LWC 47-55 °C; Ta BS/BU 7 °C/ 6 °C.","(1) - Misurata con LWC 47-55 °C; Ta BS/BU 7 °C/ 6 °C.","(1) - Misurata con LWC 47-55 °C; Ta BS/BU 7 °C/ 6 °C."]
["","","","","","(2) - Misurata con LWC 12-7 °C; Ta 35 °C.","(2) - Misurata con LWC 12-7 °C; Ta 35 °C.","(2) - Misurata con LWC 12-7 °C; Ta 35 °C."]
["","","","","","(3) - Tubazione locale 1 1/4\"","(3) - Tubazione locale 1 1/4\"","(3) - Tubazione locale 1 1/4\""]
["","","","","","(4) - Tubazione locale 1 1/2\"","(4) - Tubazione locale 1 1/2\"","(4) - Tubazione locale 1 1/2\""]