{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH"]
[]
[]
[]
[]
["","","","","","ERGA06EAV3H"]
["Dimensioni","Unità","","Altezza","mm","740"]
["","","","Larghezza","mm","884"]
["","","","Profondità","mm","388"]
["Peso","Unità","","","kg","58.5"]
["Campo di funz.","Raffresc.","","Min.","°CBS","10"]
["","","","Max.","°CBS","43"]
["Campo di funzionamento","Acqua calda sanitaria","","Min.","°CBS","-25"]
["Campo di funz.","Acqua calda sanitaria","","Max.","°CBS","35"]
["Livello potenza sonora","Riscaldamento","","Nom.","dBA","60 (1)"]
["","Raffrescamento","","Nom.","dBA","62 (1)"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","47 (1)"]
["","Raffrescamento","","Nom.","dBA","49 (1)"]
["Refrigerante","Tipo","","","","R-32"]
["","GWP","","","","675.0"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","1.01"]
["","Carica","","","kg","1.50"]
["Attacchi tubazioni","Liquido","","DE","mm","6"]
["","Gas","","DE","mm","15.9"]
["Collegamenti tubazioni","Scarico","","DE","mm","18"]
["","Dislivello","int. - est.","Max.","m","30.0"]
["Attacchi tubazioni","Isolamento termico","","","","Sulla linea del liquido e su quella del gas"]
["Alimentazione","Nome","","","","V3"]
["","Fase","","","","1N~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","230"]
["Corrente","Fusibili consigliati","","","A","20"]
["Note","","","","","(1) - Ta raffreddamento 35°C - LWE 18°C (DT=5°C) - Ta riscaldamento BS/BU 7°C/6°C - LWC 35°C (DT = 5°C)"]