{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZAG-A"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / RZAG35A2V1B","FBA50A2VEB9 / RZAG35A2V1B","FBA50A2VEB9 / RZAG50A2V1B","FBA71A2VEB9 / RZAG60A2V1B","FBA60A2VEB9 / RZAG50A2V1B","FBA60A2VEB9 / RZAG60A2V1B"]
["Capacità di Raffrescamento","Min.","","kW","1.6","1.6","1.7","1.7","1.7","1.7"]
["","Max.","","kW","5.0","5.0","6.0","7.0","6.0","7.0"]
["","Nom.","","kW","3.5","3.5","5.0","6.00","5.0","6.0"]
["Raffrescamento ambienti","SEER","","","6.12","6.17","6.30","6.25","6.63","6.15"]
["","Consumi energetici annuali","","kWh/a","200","199","278","336","264","341"]
["","Capacità","Pdesign","kW","3.50","3.50","5.00","6.00","5.00","6.00"]
["","Classe di efficienza energetica","","","A++","A++","A++","A++","A++","A++"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Capacità","Pdesign","kW","4.20","4.20","4.30","4.50","4.30","4.50"]
["","SCOP/A","","","4.10","4.14","4.10","4.18","4.28","4.10"]
["","Classe di efficienza energetica","","","A+","A+","A+","A+","A+","A+"]
["","Consumi energetici annuali","","kWh/a","1,434","1,420","1,469","1,508","1,406","1,537"]
["Efficienza nominale","Consumo energetico annuale","","kWh","389","379","625","696","608","741"]
["","EER","","","4.50","4.62","4.00","4.31","4.11","4.05"]
["","COP","","","4.40","4.44","3.80","3.87","3.97","3.80"]
["","Classe energetica","Raffreddamento","","A","A","A","A","A","A"]
["","","Riscaldamento","","A","A","A","A","A","C"]
["Capacità di riscaldamento","Nom.","","kW","4.00","4.00","6.00","7.00","6.00","7.00"]
["","Min.","","kW","1.40","1.40","1.70","1.70","1.70","1.70"]
["","Max.","","kW","5.00","5.00","6.00","7.50","6.00","7.50"]