{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":12,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG125GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Capacità di Raffrescamento","Nom.","","kW","","","6.80 (1)","","","","","13.4 (1)"]
["Raffrescamento ambienti","SEER","","","","6.91","6.91","","","","","6.75"]
["","ηs,c","","%","","","","","","","","266.9"]
["","Consumi energetici annuali","","kWh/a","","345","345","","","","","1,191"]
["","Capacità","Pdesign","kW","","6.80","6.80","","","","","13.4"]
["","Classe di efficienza energetica","","","","A++","A++"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Capacità","Pdesign","kW","","7.60","7.60","","","","","11.8"]
["","SCOP/A","","","","4.54","4.54","","","","","4.38"]
["","Classe di efficienza energetica","","","","A+","A+"]
["","Consumi energetici annuali","","kWh/a","","2,344","2,344","","","","","3,766"]
["","ηs,h","","%","","","","","","","","172.1"]
["Efficienza nominale","Consumo energetico annuale","","kWh","","","830"]
["","EER","","","","","4.09 (3)","","","","","3.18 (3)"]
["","COP","","","","","4.80 (3)","","","","","4.12 (3)"]
["","Classe energetica","Raffreddamento","","","","A"]
["","","Riscaldamento","","","","A"]
["Capacità di riscaldamento","Nom.","","kW","","","7.50 (2)","","","","","15.5 (2)"]
["Intervallo di efficienza energetica","","","","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Note","","","","","","(1) - Raffreddamento: temp. interna 27°CBS, 19°CBU, temp. esterna 35°CBS; lunghezza equivalente delle tubazioni: 7,5m; dislivello: 0m","","","","","(1) - Raffreddamento: temp. interna 27°CBS, 19°CBU, temp. esterna 35°CBS; lunghezza equivalente delle tubazioni: 7,5m; dislivello: 0m"]
["","","","","","","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 7,5m; dislivello: 0m","","","","","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 7,5m; dislivello: 0m"]
["","","","","","","(3) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","","","","","(3) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["Unità esterna","","","","","","","RZQG100L8Y1","RZQG100L8Y1","RZQG125L8Y1","RZQG125L8Y1"]
["Raffrescamento ambienti","Classe di efficienza energetica","","","","","","A","A++","A","A++"]
["","Capacità","Pdesign","kW","","","","9.50","9.50","12.0","12.0"]
["","SEER","","","","","","5.10","7.00","5.10","6.61"]
["","Consumi energetici annuali","","kWh/a","","","","652","475","824","636"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Classe di efficienza energetica","","","","","","A","A++","A","A++"]
["","Capacità","Pdesign","kW","","","","11.30","11.30","12.71","12.66"]
["","SCOP/A","","","","","","3.80","4.80","3.80","4.63"]
["","Pdh Capacità di riscaldamento a -10°","","kW","","","","9.66","9.69","11.4","11.5"]
["","Consumi energetici annuali","","kWh/a","","","","4164","3296","4683","3829"]