{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Capacità di Raffrescamento","Capacità totale","","Nom.","kW","12.10","19.00","22.00"]
["Capacità di riscaldamento","Capacità totale","","Nom.","kW","13.50","22.4","24.0"]
["Rivestimento","Colore","","","","Non verniciato","Non verniciato","Non verniciato"]
["","Materiale","","","","Acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato"]
["Dimensioni","Unità","","Altezza","mm","300","470","470"]
["","","","Larghezza","mm","1,400","1,490","1,490"]
["","","","Profondità","mm","700","1,100","1,100"]
["Peso","Unità","","","kg","45","104","115"]
["Altezza a soffitto richiesta >","mm","","","","350"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","39.0","64.0","69.0"]
["","","","Medio","m³/min","","50","56"]
["","","","Bassa","m³/min","28.0","36.0","43.0"]
["","","Riscaldamento","Alta","m³/min","39.0","64.0","69.0"]
["","","","Medio","m³/min","","50.0","56.0"]
["","","","Bassa","m³/min","28.0","36.0","43.0"]
["","Prevalenza","","Alta","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Raffrescamento","","","dBA","66","69.0","71.0"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","40","43.0","44.0"]
["","","","Medio","dBA","","39.0","40.0"]
["","","","Bassa","dBA","33","36.0","37.0"]
["","Riscaldamento","","Alta","dBA","40","43.0","44.0"]
["","","","Medio","dBA","","39.0","40.0"]
["","","","Bassa","dBA","33","36.0","37.0"]
["Attacchi tubazioni","Liquido","","DE","mm","9.52","9.52","9.52"]
["","Gas","","DE","mm","15.90","19.1","22.2"]
["","Scarico","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Prevalenza di scarico condensa","mm","","","","625"]
["Pannello decorativo","Modello","","","","BYBS125DJW1"]
["","Colore","","","","Bianco (10Y9/0,5)"]
["","Dimensioni","","Altezza","mm","55"]
["","","","Larghezza","mm","1,500"]
["","","","Profondità","mm","500"]
["","Peso","","","kg","6.5"]
["Sistemi di comando","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accessori standard","Manuale d’uso","","","","","1","1"]
["","Manuale di installazione e uso","","","","1","1","1"]
["","Manuale di installazione","","","","","1","1"]
["","Misure di sicurezza generali","","","","1","1","1"]
["","Attacco tubazione del gas","","","","","1","1"]
["","Materiale di fissaggio cavi","","","","","1","1"]
["","Rondella","","","","8","12","12"]
["","Rondella elastica","","","","","2","2"]
["","Vite+Rondella","","","","","45","45"]
["","Vite a esagono e rondella","","","","","49","49"]
["","Viti","","","","16","2","2"]
["","Vite a esagono","","","","","2","2"]
["","Rondella piana","","","","","8","8"]
["Power supply","Nome","","","","","VE","VE"]
["","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50/60","50/60","50/60"]
["","Tensione","","","V","220-240/220","220-240/220","220-240/220"]
["Accessori standard","Fascetta tubo flessibile","","","","1"]
["","Tubo flessibile di scarico","","","","1"]
["","Cavo per alimentazione comune","","","","2"]
["","Materiale sigillante (tubo di scarico)","","","","1"]
["","Materiale sigillante","","","","2"]
["","Tubo isolamento termico (liquido)","","","","1"]
["","Tubo isolamento termico (gas)","","","","1"]
["Note","","","","","(1) - Consultare i disegni separati per i dati elettrici"]