{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-C"]
[]
[]
[]
[]
["","","","","FDQ250B8V3B9 / RZQ250C7Y1B"]
["Capacità di Raffrescamento","Nom.","","kW","24.1 (1)"]
["Capacità di riscaldamento","Nom.","","kW","26.4 (2)"]
["Efficienza nominale","Consumo energetico annuale","","kWh","4,290"]
["","COP","","","3.21"]
["","EER","","","2.81"]
["Collegamenti tubazioni","Gas","DE","mm","22.2"]
["","Liquido","DE","mm","12.70"]
["Note","","","","(1) - Raffreddamento: temp. interna 27°CBS, 19,0°CBU / temp. esterna 35°CBS; lunghezza equivalente delle tubazioni: 5m; dislivello: 0m"]
["","","","","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 5m; dislivello: 0m"]
["","","","","(3) - Efficienza nominale: raffrescamento a 35°/27° carico nominale, riscaldamento a 7°/20° carico nominale"]