{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","38"]
["","","Medio","dBA","36"]
["","","Bassa","dBA","30"]
["","Raffrescamento","Medio","dBA","36"]
["","","Bassa","dBA","30"]
["","","Alta","dBA","38"]
["Accessori standard","Manuale di installazione","","","1"]
["","Manuale d’uso","","","1"]
["","Isolante per il collegamento","","","1"]
["","Materiale di tenuta","","","1"]
["","Fascetta metallica","","","1"]
["","Tubo flessibile di scarico","","","1"]
["","Rondella per staffa di sospensione","","","8"]
["","Materiale sigillante","","","2"]
["","Fascette","","","6"]
["","Piastra di fissaggio rondella","","","4"]
["","Viti per flange canalizzazione","","","1"]
["","Filtro aria","","","1"]
["Attacchi tubazioni","Liquido","DE","mm","6.35"]
["","Gas","DE","mm","12.7"]
["","Scarico","","","VP20 (I.D. 20/O.D. 26)"]
["Potenza assorbita","Raffrescamento","Nom.","kW","0.060"]
["","Riscaldamento","Nom.","kW","0.060"]
["Sound power level","Raffrescamento","","dBA","55"]
["","Riscaldamento","","dBA","55"]
["Dimensioni","Unità","Larghezza","mm","1,150"]
["","","Profondità","mm","620"]
["","","Altezza","mm","200"]
["Peso","Unità","","kg","30.0"]
["Ventilatore","Prevalenza","Nom.","Pa","40"]
["Power supply","Fase","","","1~"]
["","Frequenza","","Hz","50/60"]
["","Nome","","","VE"]
["","Tensione","","V","220-240"]
["Note","","","","(1) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare."]