{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Rivestimento","Materiale","","","","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato"]
["Dimensioni","Unità","","Altezza","mm","260","260","260","260"]
["","","","Larghezza","mm","575","575","575","575"]
["","","","Profondità","mm","575","575","575","575"]
["Peso","Unità","","","kg","16.0","16.0","17.5","17.5"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³;/min","9.0","10.0","12.0","14.5"]
["","","","Medio","m³;/min","8.0","8.5","10.0","12.5"]
["","","","Bassa","m³;/min","6.5","6.5","7.5","9.5"]
["","","Riscaldamento","Alta","m³;/min","9.0","10.0","12.0","14.5"]
["","","","Medio","m³;/min","8.0","8.5","10.0","12.5"]
["","","","Bassa","m³;/min","6.5","6.5","7.5","9.5"]
["Potenza sonora","Raffrescamento","","","dBA","48","51","56","60"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","31.0","34.0","39.0","43.0"]
["Pressione sonora","Raffrescamento","","Medio","dBA","28.5","30.5","34.0","40.0"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","25.0","25.0","27.0","32.0"]
["","Riscaldamento","","Alta","dBA","31.0","34.0","39.0","43.0"]
["Pressione sonora","Riscaldamento","","Medio","dBA","28.5","30.5","34.0","40.0"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","25.0","25.0","27.0","32.0"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35","6.35","6.35"]
["","Gas","","DE","mm","9.52","9.52","12.70","12.70"]
["","Scarico","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Pannello decorativo","Modello","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Colore","","","","Bianco (N9.5)","Bianco (N9.5)","Bianco (N9.5)","Bianco (N9.5)"]
["","Dimensioni","","Altezza","mm","46","46","46","46"]
["","","","Larghezza","mm","620","620","620","620"]
["","","","Profondità","mm","620","620","620","620"]
["","Peso","","","kg","2.8","2.8","2.8","2.8"]
["Pannello decorativo 2","Modello","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Colore","","","","Argento","Argento","Argento","Argento"]
["","Dimensioni","","Altezza","mm","46","46","46","46"]
["","","","Larghezza","mm","620","620","620","620"]
["","","","Profondità","mm","620","620","620","620"]
["","Peso","","","kg","2.8","2.8","2.8","2.8"]
["Pannello decorativo 3","Modello","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Colore","","","","Bianco (RAL9010)","Bianco (RAL9010)","Bianco (RAL9010)","Bianco (RAL9010)"]
["","Dimensioni","","Altezza","mm","55","55","55","55"]
["","","","Larghezza","mm","700","700","700","700"]
["","","","Profondità","mm","700","700","700","700"]
["","Peso","","","kg","2.7","2.7","2.7","2.7"]
["Pannello decorativo 4","Modello","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Colore","","","","Bianco (RAL9010)","Bianco (RAL9010)","Bianco (RAL9010)","Bianco (RAL9010)"]
["","Dimensioni","","Altezza","mm","55","55","55","55"]
["","","","Larghezza","mm","700","700","700","700"]
["","","","Profondità","mm","700","700","700","700"]
["","Peso","","","kg","2.7","2.7","2.7","2.7"]
["Sistemi di controllo","Telecomando infrarossi","","","","BRC7EB530 (pannello standard), BRC7F530W (pannello bianco), BRC7F530S (pannello grigio)","BRC7EB530 (pannello standard), BRC7F530W (pannello bianco), BRC7F530S (pannello grigio)","BRC7EB530 (pannello standard), BRC7F530W (pannello bianco), BRC7F530S (pannello grigio)","BRC7EB530 (pannello standard), BRC7F530W (pannello bianco), BRC7F530S (pannello grigio)"]
["","Telecomando con cavo","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Accessori standard","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Alimentazione","Fase","","","","1~","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240","220-240"]