{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":17,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA60AVEB / FHA60AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG71L8Y1B","FHA71AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA71AVEB / FHA71AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA71AVEB / FHA71AVEB / RZQG125L8Y1B"]
["Intervallo di efficienza energetica","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","","","","","A+++ ~ D"]
["Raffrescamento ambienti","SEER","","","","","","","","5.10","6.86","5.10","5.10","5.10","5.10","5.10"]
["","Consumi energetici annuali","","kWh/a","","","","","","467","347","467","467","652","652","652"]
["","Capacità","Pdesign","kW","","","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50"]
["","Classe di efficienza energetica","","","","","","","","A","A++","A","A","A","A","A"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Capacità","Pdesign","kW","","","","","","6.00","7.60","6.00","6.00","11.30","11.30","11.30"]
["","SCOP/A","","","","","","","","3.80","4.32","3.80","3.80","3.80","3.80","3.80"]
["","Classe di efficienza energetica","","","","","","","","A","A+","A","A","A","A","A"]
["","Consumi energetici annuali","","kWh/a","","","","","","2,211","2,463","2,211","2,211","4,164","4,164","4,164"]
["Capacità di Raffrescamento","Nom.","","kW","","","","","","","6.80 (1)"]
["Efficienza nominale","Consumo energetico annuale","","kWh","","","","","","","890"]
["","EER","","","","","","","","","3.82 (3)"]
["","COP","","","","","","","","","4.13 (3)"]
["","Classe energetica","Raffreddamento","","","","","","","","A"]
["","","Riscaldamento","","","","","","","","A"]
["Capacità di riscaldamento","Nom.","","kW","","","","","","","7.50 (2)"]
["Note","","","","","","","","","","(1) - Raffreddamento: temp. interna 27°CBS, 19°CBU, temp. esterna 35°CBS; lunghezza equivalente delle tubazioni: 7,5m; dislivello: 0m","(1) - Raffreddamento: temp. interna 27°CBS, 19°CBU, temp. esterna 35°CBS; lunghezza equivalente delle tubazioni: 7,5m; dislivello: 0m"]
["","","","","","","","","","","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 7,5m; dislivello: 0m","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 7,5m; dislivello: 0m"]
["","","","","","","","","","","(3) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE","(3) - Valori EER/COP conformi allo standard Eurovent 2012, solo per l'uso fuori dall'UE"]
["Raffrescamento ambienti","Classe di efficienza energetica","","","","","","","","","","","","","","","A"]
["","Capacità","Pdesign","kW","","","","","","","","","","","","","12.00"]
["","SEER","","","","","","","","","","","","","","","5.10"]
["","Consumi energetici annuali","","kWh/a","","","","","","","","","","","","","824"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Classe di efficienza energetica","","","","","","","","","","","","","","","A"]
["","Capacità","Pdesign","kW","","","","","","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","","","","","","3.80"]
["","Pdh Capacità di riscaldamento a -10°","","kW","","","","","","","","","","","","","11"]
["","Consumi energetici annuali","","kWh/a","","","","","","","","","","","","","4683"]