{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","42","44","46","39","40","41"]
["","","Funzionamento silenzioso","dBA","30","32","34","25","25","26"]
["","","Bassa","dBA","33","35","37","28","28","29"]
["","Raffrescamento","Funzionamento silenzioso","dBA","31","33","34","22","22","23"]
["","","Bassa","dBA","34","36","37","25","26","27"]
["","","Alta","dBA","43","45","46","39","40","41"]
["","","Nom.","dBA","38","40","42","34","34","35"]
["","Raffrescamento","Nom.","dBA","39","41","42","33","33","34"]
["Accessori standard","Filtro purificatore d'aria a base di apatite e titanio","","","2","2","2","2","2","2"]
["","Manuale d’uso","","","1","1","1","1","1","1"]
["","Manuale di installazione","","","1","1","1","1","1","1"]
["","Telecomando ad infrarossi","","","1","1","1","1","1","1"]
["","Batterie","","","2","2","2","2","2","2"]
["","Supporto del telecomando","","","1","1","1","1","1","1"]
["","Piastra di montaggio","","","1","1","1","1","1","1"]
["","Viti di fissaggio unità interna","","","2","2"]
["Sistemi di controllo","Infrared remote control","","","ARC433B70","ARC433B70","ARC433B70"]
["Attacchi tubazioni","Liquido","DE","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","DE","mm","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Scarico","","","18","18","18","18","18","18"]
["Potenza assorbita","Raffrescamento","Nom.","kW","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Riscaldamento","Nom.","kW","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Livello potenza sonora","Raffrescamento","","dBA","59","60","63","55","56","57"]
["","Riscaldamento","","dBA","58","59","62","55","56","57"]
["Dimensioni","Unità","Larghezza","mm","1,050","1,050","1,050","770","770","770"]
["","","Profondità","mm","238","238","238","198","198","198"]
["","","Altezza","mm","290","290","290","283","283","283"]
["Rivestimento","Colour","","","Bianco","Bianco","Bianco","Bianco","Bianco","Bianco"]
["Peso","Unità","","kg","12","12","12","7","7","7"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Frequenza","","Hz","50","50","50","50","50","50"]
["","Nome","","","V1","V1","V1","V1","V1","V1"]
["","Tensione","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Note","","","","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["Accessori standard","Viti di fissaggio unità interna (M4 x 12L)","","","","","2"]
["","Vite di fissaggio per unità interna","","","","","","2","2","2"]