{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","39","40","41","","46"]
["","","","Medio","dBA","32","33","33","","42"]
["","","","Funzionamento silenzioso","dBA","19","19","19","","24"]
["","","","Bassa","dBA","25","25","25","","33"]
["","Raffrescamento","","Medio","dBA","32","33","33","","39"]
["","","","Funzionamento silenzioso","dBA","19","19","19","","24"]
["","","","Bassa","dBA","25","25","25","","31"]
["","","","Alta","dBA","39","40","41","","46"]
["Accessori standard","Manuale di installazione","","","","1","1","1","","1"]
["","Manuale d’uso","","","","1","1","1","","1"]
["","Filtro aria","","","","2","2","2","","2"]
["","Telecomando a raggi infrarossi","","","","1","1","1","","1"]
["","Piastra di fissaggio del telecomando","","","","1","1","1","","1"]
["","Sacchetto viti","","","","1","1","1","","1"]
["","Coprivite","","","","1","1","1","","1"]
["","Batterie a secco AAA","","","","2","2","2","","2"]
["","Misure di sicurezza generali","","","","1","1","1","","1"]
["Refrigerante","GWP","","","","675.0","675.0","675.0","","675.0"]
["Sistemi di comando","Telecomando con cavo","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Piping connections","Liquido","","DE","mm","6.35","6.35","6.35","","6.35"]
["","Gas","","DE","mm","9.50","9.50","9.50","","12.70"]
["","Scarico","","","","18","18","18","","18"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Riscaldamento","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Livello di potenza sonora","Raffrescamento","","","dBA","57","57","60","","60"]
["Dimensioni","Unità","","Larghezza","mm","798","798","798","","798"]
["","","","Profondità","mm","189","189","189","","189"]
["","","","Altezza","mm","295","295","295","","295"]
["Casing","Colour","","","","Bianco","Bianco","Bianco","","Bianco"]
["Peso","Unità","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilatore","Portata d'aria","Riscaldamento","Alta","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Medio","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Bassa","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Funzionamento silenzioso","m³/min","4.5","4.5","4.5","","5.7"]
["","","Raffrescamento","Bassa","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Medio","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Alta","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Funzionamento silenzioso","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Phase","","","","1~","1~","1~","","1~"]
["","Nome","","","","V1","V1","V1","","V1"]
["","Frequenza","","","Hz","50","50","50","","50"]
["","Tensione","","","V","220-240","220-240","220-240","","220-240"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","","","0.028"]
["","Riscaldamento","","Nom.","kW","","","","0.036"]
["Rivestimento","Colore","","","","","","","Bianco"]
["Dimensioni","Unità","","Altezza","mm","","","","295"]
["","","","Larghezza","mm","","","","798"]
["","","","Profondità","mm","","","","189"]
["Peso","Unità","","","kg","","","","11.50"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","","","13.1"]
["","","","Medio","m³/min","","","","9.8"]
["","","","Bassa","m³/min","","","","7.2"]
["","","","Funzionamento silenzioso","m³/min","","","","4.6"]
["","","Riscaldamento","Alta","m³/min","","","","14.6"]
["","","","Medio","m³/min","","","","10.5"]
["","","","Bassa","m³/min","","","","7.7"]
["","","","Funzionamento silenzioso","m³/min","","","","5.2"]
["Potenza sonora","Raffrescamento","","","dBA","","","","60"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","","","45"]
["Pressione sonora","Raffrescamento","","Medio","dBA","","","","37"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","","","","29"]
["","","","Funzionamento silenzioso","dBA","","","","21"]
["","Riscaldamento","","Alta","dBA","","","","45"]
["Pressione sonora","Riscaldamento","","Medio","dBA","","","","37"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","","","","29"]
["","","","Funzionamento silenzioso","dBA","","","","21"]
["Refrigerante","GWP","","","","","","","675.0"]
["Attacchi tubazioni","Liquido","","DE","mm","","","","6.35"]
["","Gas","","DE","mm","","","","12.70"]
["","Scarico","","","","","","","18"]
["Sistemi di controllo","Telecomando infrarossi","","","","","","","ARC466A58"]
["","Telecomando con cavo","","","","","","","BRC073"]
["Accessori standard","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Air filter","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Alimentazione","Nome","","","","","","","V1"]
["","Fase","","","","","","","1~"]
["","Frequenza","","","Hz","","","","50"]
["","Tensione","","","V","","","","220-240"]