{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":10,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-DG"]
[]
[]
[]
[]
["","","","","","FTXA20D2V1BG","FTXA25D2V1BG","FTXA35D2V1BG","FTXA42D2V1BG","FTXA50D2V1BG"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.020","0.022","0.023","0.028","0.030"]
["","Riscaldamento","","Nom.","kW","0.020","0.020","0.220","0.036","0.039"]
["Rivestimento","Colore","","","","Casing: Black, Panel: Grey fabric","Casing: Black, Panel: Grey fabric","Casing: Black, Panel: Grey fabric","Casing: Black, Panel: Grey fabric","Casing: Black, Panel: Grey fabric"]
["Dimensioni","Unità","","Altezza","mm","295","295","295","295","295"]
["","","","Larghezza","mm","798","798","798","798","798"]
["","","","Profondità","mm","189","189","189","189","189"]
["Peso","Unità","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","11.0","11.5","11.9","13.1","13.5"]
["","","","Medio","m³/min","8.2","8.6","8.6","9.8","10.4"]
["","","","Bassa","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Funzionamento silenzioso","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Riscaldamento","Alta","m³/min","10.9","11.1","11.5","14.6","15.1"]
["","","","Medio","m³/min","8.7","9.0","9.0","10.5","11.1"]
["","","","Bassa","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Funzionamento silenzioso","m³/min","4.5","4.5","4.5","5.2","5.7"]
["Potenza sonora","Raffrescamento","","","dBA","57","57","60","60","60"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","39","40","41","45","46"]
["Pressione sonora","Raffrescamento","","Medio","dBA","32","33","33","37","39"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","25","25","25","29","31"]
["","","","Funzionamento silenzioso","dBA","19","19","19","21","24"]
["","Riscaldamento","","Alta","dBA","39","40","41","45","46"]
["Pressione sonora","Riscaldamento","","Medio","dBA","32","33","33","37","42"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","25","25","25","29","33"]
["","","","Funzionamento silenzioso","dBA","19","19","19","21","24"]
["Refrigerante","GWP","","","","675.0","675.0","675.0","675.0","675.0"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","DE","mm","9.50","9.50","9.50","9.50","12.7"]
["","Scarico","","","","18","18","18","18","18"]
["Sistemi di controllo","Telecomando infrarossi","","","","ARC466A94","ARC466A94","ARC466A94","ARC466A94","ARC466A94"]
["","Telecomando con cavo","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Accessori standard","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Filtro aria","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Intervallo di efficienza energetica","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Alimentazione","Nome","","","","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240","220-240","220-240"]