{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","39","40"]
["","","Medio","dBA","34","34"]
["","","Funzionamento silenzioso","dBA","21","21"]
["","","Bassa","dBA","28","28"]
["","Raffrescamento","Medio","dBA","33","33"]
["","","Funzionamento silenzioso","dBA","20","20"]
["","","Bassa","dBA","25","26"]
["","","Alta","dBA","39","40"]
["Accessori standard","Manuale di installazione","","","1","1"]
["","Manuale d’uso","","","1","1"]
["","Telecomando a raggi infrarossi","","","1","1"]
["","Batterie a secco AAA","","","2","2"]
["","Supporto del telecomando","","","1","1"]
["","Piastra di montaggio","","","1","1"]
["","Viti di fissaggio unità interna","","","2","2"]
["Sistemi di controllo","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Piping connections","Liquido","DE","mm","6.35","6.35"]
["","Gas","DE","mm","9.50","9.50"]
["","Scarico","","","18","18"]
["Potenza assorbita","Raffrescamento","Nom.","kW","0.017","0.019"]
["","Riscaldamento","Nom.","kW","0.020","0.020"]
["Livello potenza sonora","Raffrescamento","","dBA","55","55"]
["","Riscaldamento","","dBA","55","55"]
["Dimensioni","Unità","Larghezza","mm","770","770"]
["","","Profondità","mm","225","225"]
["","","Altezza","mm","286","286"]
["Rivestimento","Colour","","","Bianco","Bianco"]
["Peso","Unità","","kg","8.50","8.50"]
["Power supply","Phase","","","1~","1~"]
["","Frequenza","","Hz","50","50"]
["","Tensione","","V","220-240","220-240"]