{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":7,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JB"]
[]
[]
[]
[]
["","","","","FTXG25JV1BB","FTXG35JV1BB","FTXG50JV1BB"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","39","42","44"]
["","","Funzionamento silenzioso","dBA","25","26","32"]
["","","Bassa","dBA","28","29","35"]
["","Raffrescamento","Funzionamento silenzioso","dBA","22","23","32"]
["","","Bassa","dBA","25","26","35"]
["","","Alta","dBA","38","42","44"]
["","","Nom.","dBA","34","36","40"]
["","Raffrescamento","Nom.","dBA","32","34","40"]
["Accessori standard","Filtro purificatore d'aria a base di apatite e titanio","","","2","2","2"]
["","Manuale d’uso","","","1","1","1"]
["","Manuale di installazione","","","1","1","1"]
["","Telecomando ad infrarossi","","","1","1","1"]
["","Batterie","","","2","2","2"]
["","Supporto del telecomando","","","1","1","1"]
["","Viti di fissaggio unità interna","","","2","2","2"]
["","Piastra di montaggio","","","1","1","1"]
["","Maschera in carta","","","2","2","2"]
["Attacchi tubazioni","Liquido","DE","mm","6.35","6.35","6.35"]
["","Gas","DE","mm","9.52","9.52","12.7"]
["","Scarico","","","16 o 18","16 o 18","18"]
["Potenza assorbita","Raffrescamento","Nom.","kW","0.018 (3), 0.018 (4), 0.018 (5)","0.026 (3), 0.026 (4), 0.026 (5)","0.032 (3), 0.032 (4), 0.032 (5)"]
["","Riscaldamento","Nom.","kW","0.024 (3), 0.024 (4), 0.024 (5)","0.032 (3), 0.032 (4), 0.032 (5)","0.038 (3), 0.038 (4), 0.038 (5)"]
["Livello potenza sonora","Raffrescamento","","dBA","56","60","60"]
["","Riscaldamento","","dBA","57","60","60"]
["Dimensioni","Unità","Larghezza","mm","915","915","915"]
["","","Profondità","mm","155","155","155"]
["","","Altezza","mm","295","295","295"]
["Rivestimento","Colore","","","Nero opaco","Nero opaco","Nero opaco"]
["Peso","Unità","","kg","11","11","11"]
["Power supply","Fase","","","1~","1~","1~"]
["","Frequenza","","Hz","50","50","50"]
["","Nome","","","V1","V1","V1"]
["","Tensione","","V","220-240","220-240","220-240"]
["Note","","","","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria"]
["","","","","(2) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare.","(2) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare.","(2) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare."]
["","","","","(3) - 220V","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230V","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V","(5) - 240V"]