{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-K"]
[]
[]
[]
[]
["","","","","FTXM20K3V1B (Archived)","FTXM25K3V1B (Archived)","FTXM35K3V1B (Archived)","FTXM42K3V1B (Archived)","FTXM50K3V1B (Archived)"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","40","41","45","45","47"]
["","","Funzionamento silenzioso","dBA","19","19","19","22","24"]
["","","Bassa","dBA","27","27","29","33","34"]
["","Raffrescamento","Funzionamento silenzioso","dBA","19","19","19","21","23"]
["","","Bassa","dBA","24","25","29","33","34"]
["","","Alta","dBA","40","41","45","45","46"]
["","","Nom.","dBA","34","34","39","39","40"]
["","Raffrescamento","Nom.","dBA","32","33","37","39","40"]
["Accessori standard","Manuale d’uso","","","1","1","1","1","1"]
["","Manuale di installazione","","","1","1","1","1","1"]
["","Telecomando a raggi infrarossi","","","1","1","1","1","1"]
["","Batterie","","","2","2","2","2","2"]
["","Piastra di montaggio","","","1","1","1","1","1"]
["","Viti di fissaggio unità interna","","","2","2","2","2","2"]
["","Filtro purificatore d'aria a base di apatite e titanio","","","2","2","2","2","2"]
["","Supporto del telecomando","","","1","1","1","1","1"]
["Sistemi di comando","Infrared remote control","","","ARC466A6","ARC466A6","ARC466A9","ARC466A9","ARC466A9"]
["Collegamenti tubazioni","Liquido","DE","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","DE","mm","9.5","9.5","9.5","12.7","12.7"]
["","Scarico","","","18","18","18","18","18"]
["Sound power level","Raffrescamento","","dBA","56","57","59","59","60"]
["","Riscaldamento","","dBA","56","57","59","59","60"]
["Dimensioni","Unità","Larghezza","mm","780","780","900","900","900"]
["","","Profondità","mm","215","215","215","215","215"]
["","","Altezza","mm","289","289","298","298","298"]
["Rivestimento","Colore","","","Bianco","Bianco","Bianco","Bianco","Bianco"]
["Peso","Unità","","kg","8","8","11","11","11"]
["Power supply","Fase","","","1~","1~","1~","1~","1~"]
["","Frequenza","","Hz","50","50","50","50","50"]
["","Nome","","","V1","V1","V1","V1","V1"]
["","Tensione","","V","220-240","220-240","220-240","220-240","220-240"]
["Note","","","","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]