{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 2MXM-M9"]
[]
[]
[]
[]
["","","","","FTXM25M2V1B / FTXM42M2V1B / 2MXM50M2V1B9"]
["Capacità di Raffrescamento","Nom.","","kW","5.0"]
["Efficienza nominale","Consumo energetico annuale","","kWh","612"]
["","EER","","","4.09"]
["","COP","","","4.03"]
["","Classe energetica","Raffreddamento","","A"]
["","","Riscaldamento","","A"]
["Capacità di riscaldamento","Min.","","kW","5.60"]
["Note","","","","(1) - Le capacità di raffreddamento nominali si riferiscono a: temperatura interna: 27°CBS, 19°CBU, temperatura esterna: 35°CBS / lunghezza equivalente del circuito frigorifero: 5m, dislivello: 0m. Dati per la serie ad efficienza standard. Tolleranze usate Eurovent 2015."]
["","","","","(2) - Le capacità di riscaldamento nominali si riferiscono a: temperatura interna: 20°CBS, temperatura esterna: 7°CBS, 6°CBU, lunghezza equivalente delle tubazioni: 5m, dislivello: 0m."]