{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / RXM-M9"]
[]
[]
[]
[]
["","","","","FTXM20M2V1B / RXM20M3V1B9","FTXM25M2V1B / RXM25M3V1B9","FTXM35M2V1B / RXM35M3V1B9","FTXM42M2V1B / RXM42M3V1B9","FTXM50M2V1B / RXM50M3V1B9","FTXM60M2V1B / RXM60M3V1B9"]
["Capacità di Raffrescamento","Min.","","kW","1.3"]
["","Max.","","kW","2.6"]
["","Nom.","","kW","2.0"]
["Efficienza nominale","Consumo energetico annuale","","kWh","220"]
["","EER","","","4.57"]
["","COP","","","5.00"]
["","Classe energetica","Raffreddamento","","A"]
["","","Riscaldamento","","A"]
["Capacità di riscaldamento","Nom.","","kW","2.50"]
["","Min.","","kW","1.30"]
["","Max.","","kW","3.50"]
["Note","","","","(1) - Consultare i disegni separati per i dati elettrici"]
["","","","","(2) - Le capacità di raffrescamento nom. si riferiscono a: temperatura interna: 27°CBS, 19°CBU, temperatura esterna: 35°CBS, lunghezza equivalente delle tubazioni del refrigerante: 5m, dislivello: 0m."]
["","","","","(3) - Le capacità di riscaldamento nominali si riferiscono a: temperatura interna: 20°CBS, temperatura esterna: 7°CBS, 6°CBU, lunghezza equivalente delle tubazioni: 5m, dislivello: 0m."]
["Outdoor unit","","","","","RXM25M3V1B9","RXM35M3V1B9","RXM42M3V1B9","RXM50M3V1B9","RXM60M3V1B9"]
["Capacità di Raffrescamento","Min.","","kW","","1.3","1.4","1.70","1.70","1.90"]
["","Capacità di Raffrescamento-=-Nom.-=-kW","","kW","","2.5","3.4","4.20","5.00","6.00"]
["","Max.","","kW","","3.2","4.0","5.00","5.30","6.70"]
["Capacità di riscaldamento","Min.","","kW","","1.30","1.40","1.70","1.70","1.70"]
["","Nom.","","kW","","2.80","4.00","5.40","5.80","7.00"]
["","Max.","","kW","","4.70","5.20","6.00","6.50","8.00"]
["Efficienza nominale","EER","","","","4.50","4.23","3.75","3.68","3.39"]
["","COP","","","","5.00","4.04","4.12","4.00","3.61"]
["","Consumo energetico annuale","","kWh","","280","400"]
["","Classe energetica","Raffreddamento","","","A","A","A","A","A"]
["","","Riscaldamento","","","A","A","A","A","A"]
["Raffrescamento ambienti","Classe di efficienza energetica","","","","A+++","A+++","A++","A++","A++"]
["","Capacità","Pdesign","kW","","2.50","3.40","4.20","5.00","6.00"]
["","SEER","","","","8.52","8.51","7.50","7.33","6.90"]
["","Consumi energetici annuali","","kWh/a","","103","140","196","239","304"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Classe di efficienza energetica","","","","A+++","A+++","A++","A++","A+"]
["","Capacità","Pdesign","kW","","2.40","2.50","4.00","4.60","4.60"]
["","SCOP/A","","","","5.10","5.10","4.60","4.60","4.30"]
["","Pdh Capacità di riscaldamento a -10°","","kW","","2.30","2.35","3.68","4.09","4.09"]
["","Consumi energetici annuali","","kWh/a","","659","686","1216","1400","1496"]