{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","38","39","42","42","44","","46"]
["","","","Funzionamento silenzioso","dBA","25","25","26","30","31","","34"]
["","","","Bassa","dBA","28","28","29","33","34","","37"]
["","Raffrescamento","","Funzionamento silenzioso","dBA","22","22","23","30","31","","34"]
["","","","Bassa","dBA","25","25","26","33","34","","37"]
["","","","Alta","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Raffrescamento","","Nom.","dBA","32","32","34","38","39","","42"]
["Accessori standard","Filtro purificatore d'aria a base di apatite e titanio","","","","2","2","2","2","2"]
["","Manuale d’uso","","","","1","1","1","1","1","","1"]
["","Manuale di installazione","","","","1","1","1","1","1","","1"]
["","Telecomando ad infrarossi","","","","1","1","1","1","1","","1"]
["","Batterie","","","","2","2","2","2","2","","2"]
["","Supporto del telecomando","","","","1","1","1","1","1","","1"]
["","Viti di fissaggio unità interna","","","","2","2","2","2","2","","2"]
["","Piastra di montaggio","","","","1","1","1","1","1","","1"]
["Sistemi di controllo","Infrared remote control","","","","","","","","","","ARC452A3"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gas","","DE","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Scarico","","","","18","18","18","18","18","","18"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Riscaldamento","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Livello potenza sonora","Raffrescamento","","","dBA","54","54","58","58","59","","63"]
["","Riscaldamento","","","dBA","54","55","58","58","60","","62"]
["Dimensioni","Unità","","Larghezza","mm","800","800","800","800","800","","1,050"]
["","","","Profondità","mm","215","215","215","215","215","","250"]
["","","","Altezza","mm","295","295","295","295","295","","290"]
["Rivestimento","Colour","","","","Bianco","Bianco","Bianco","Bianco","Bianco","","Bianco"]
["Peso","Unità","","","kg","9","9","10","10","10","","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frequenza","","","Hz","50","50","50","50","50","","50"]
["","Nome","","","","V1","V1","V1","V1","V1","","V1"]
["","Tensione","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V"]
["Ventilatore","Portata d'aria","Raffrescamento","Nom.","m³/min","","","","","","16.0"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","","","","","","41"]
["Ventilatore","Portata d'aria","Riscaldamento","Nom.","m³/min","","","","","","14.9"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","","","","","","40"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Riscaldamento","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Rivestimento","Colore","","","","","","","","","Bianco"]
["Dimensioni","Unità","","Altezza","mm","","","","","","290"]
["","","","Larghezza","mm","","","","","","1050"]
["","","","Profondità","mm","","","","","","250"]
["Peso","Unità","","","kg","","","","","","12"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","","","","","16.0"]
["","","","Bassa","m³/min","","","","","","11.3"]
["","","","Funzionamento silenzioso","m³/min","","","","","","10.1"]
["","","Riscaldamento","Alta","m³/min","","","","","","17.2"]
["","","","Bassa","m³/min","","","","","","12.6"]
["","","","Funzionamento silenzioso","m³/min","","","","","","11.3"]
["Potenza sonora","Raffrescamento","","","dBA","","","","","","60"]
["","Riscaldamento","","","dBA","","","","","","59"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","","","","","45"]
["","","","Bassa","dBA","","","","","","36"]
["","","","Funzionamento silenzioso","dBA","","","","","","33"]
["","Riscaldamento","","Alta","dBA","","","","","","44"]
["","","","Bassa","dBA","","","","","","35"]
["","","","Funzionamento silenzioso","dBA","","","","","","32"]
["Attacchi tubazioni","Liquido","","DE","mm","","","","","","6.35"]
["","Gas","","DE","mm","","","","","","12.7"]
["","Scarico","","","","","","","","","18"]
["Sistemi di controllo","Telecomando infrarossi","","","","","","","","","ARC452A3"]
["Accessori standard","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Alimentazione","Nome","","","","","","","","","V1"]
["","Fase","","","","","","","","","1~"]
["","Frequenza","","","Hz","","","","","","50"]
["","Tensione","","","V","","","","","","220-240"]
["Accessori standard","Filtro purificatore d'aria all'apatite di titanio senza telaio","","","","","","","","","","2"]
["Note","","","","","","","","","","","(4) - 240V"]