{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","40","","","","","","45"]
["","","","Funzionamento silenzioso","dBA","19","","","","","","22"]
["","","","Bassa","dBA","27","","","","","","33"]
["","Raffrescamento","","Funzionamento silenzioso","dBA","19","","","","","","21"]
["","","","Bassa","dBA","24","","","","","","33"]
["","","","Alta","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Raffrescamento","","Nom.","dBA","32","","","","","","39"]
["Accessori standard","Manuale di installazione","","","","1","","","","","","1"]
["","Manuale d’uso","","","","1","","","","","","1"]
["","Telecomando ad infrarossi","","","","1","","","","","","1"]
["","Batterie","","","","2","","","","","","2"]
["","Supporto del telecomando","","","","1","","","","","","1"]
["","Piastra di montaggio","","","","1","","","","","","1"]
["","Viti di fissaggio unità interna","","","","2","","","","","","2"]
["","Filtro purificatore d'aria a base di apatite e titanio","","","","2","","","","","","2"]
["Sistemi di comando","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","","","","","","6.35"]
["","Gas","","DE","mm","9.5","","","","","","9.5"]
["","Scarico","","","","18","","","","","","18"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Riscaldamento","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Raffrescamento","","","dBA","58","","","","","","59"]
["","Riscaldamento","","","dBA","58","","","","","","59"]
["Dimensioni","Unità","","Larghezza","mm","780","","","","","","900"]
["","","","Profondità","mm","215","","","","","","215"]
["","","","Altezza","mm","289","","","","","","298"]
["Rivestimento","Colore","","","","Bianco","","","","","","Bianco"]
["Peso","Unità","","","kg","8","","","","","","11"]
["Power supply","Fase","","","","1~","","","","","","1~"]
["","Frequenza","","","Hz","50","","","","","","50"]
["","Nome","","","","V1","","","","","","V1"]
["","Tensione","","","V","220-240","","","","","","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Riscaldamento","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Rivestimento","Colore","","","","","Bianco","Bianco","Bianco","Bianco","Bianco","","Bianco","Bianco","Bianco"]
["Dimensioni","Unità","","Altezza","mm","","215","289","215","298","215","","215","298","215"]
["","","","Larghezza","mm","","780","780","780","900","900","","900","900","900"]
["","","","Profondità","mm","","289","215","289","215","298","","298","215","298"]
["Peso","Unità","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Medio","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Bassa","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Funzionamento silenzioso","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Riscaldamento","Alta","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","","Medio","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","","Bassa","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Funzionamento silenzioso","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Potenza sonora","Raffrescamento","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Riscaldamento","","","dBA","","58","58","58","59","59","","59","60","60"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","40","41","41","45","45","","45","46","46"]
["Pressione sonora","Raffrescamento","","Medio","dBA","","32","33","33","","37","","39","","40"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Funzionamento silenzioso","dBA","","19","19","19","19","19","","21","23","23"]
["","Riscaldamento","","Alta","dBA","","40","41","41","45","45","","45","47","47"]
["Pressione sonora","Riscaldamento","","Medio","dBA","","34","34","34","","39","","39","","40"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Funzionamento silenzioso","dBA","","19","19","19","19","19","","22","24","24"]
["Attacchi tubazioni","Liquido","","DE","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gas","","DE","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Scarico","","","","","18","18","18","18","18","","18","18","18"]
["Sistemi di comando","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Accessori standard","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Alimentazione","Nome","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fase","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frequenza","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Tensione","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilatore","Portata d'aria","Raffrescamento","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilatore","Portata d'aria","Riscaldamento","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","","","34","","39","","","","40"]
["Sistemi di controllo","Telecomando infrarossi","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Accessori standard","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Note","","","","","","","","","","","(4) - 240V"]