{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BB"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","41"]
["","","","Medio","dBA","31"]
["","","","Funzionamento silenzioso","dBA","19"]
["","","","Bassa","dBA","24"]
["","Raffrescamento","","Medio","dBA","32"]
["","","","Funzionamento silenzioso","dBA","20"]
["","","","Bassa","dBA","25"]
["","","","Alta","dBA","43"]
["Accessori standard","Manuale di installazione","","","","1"]
["","Manuale d’uso","","","","1"]
["","Filtro aria","","","","2"]
["","Telecomando a raggi infrarossi","","","","1"]
["","Piastra di fissaggio del telecomando","","","","1"]
["","Sacchetto viti","","","","1"]
["","Coprivite","","","","2"]
["","Batterie a secco AAA","","","","2"]
["","Misure di sicurezza generali","","","","1"]
["Refrigerante","GWP","","","","675.0"]
["Sistemi di comando","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35"]
["","Gas","","DE","mm","9.50"]
["","Scarico","","","","18"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.023"]
["","Riscaldamento","","Nom.","kW","0.022"]
["Sound power level","Raffrescamento","","","dBA","60"]
["","Riscaldamento","","","dBA","60"]
["Dimensioni","Unità","","Larghezza","mm","798"]
["","","","Profondità","mm","189"]
["","","","Altezza","mm","295"]
["Rivestimento","Colore","","","","Nero"]
["Peso","Unità","","","kg","11.5"]
["Ventilatore","Portata d'aria","Riscaldamento","Alta","m³/min","11.5"]
["","","","Bassa","m³/min","6.0"]
["","","","Medio","m³/min","8.0"]
["","","","Funzionamento silenzioso","m³/min","5.1"]
["","","Raffrescamento","Bassa","m³/min","5.7"]
["","","","Medio","m³/min","8.3"]
["","","","Alta","m³/min","11.9"]
["","","","Funzionamento silenzioso","m³/min","4.6"]
["Power supply","Fase","","","","1~"]
["","Frequenza","","","Hz","50"]
["","Nome","","","","V1"]
["","Tensione","","","V","220-240"]
["Note","","","","","(1) - Raffreddamento: temp. interna 27°CBS, 19,0°CBU / temp. esterna 35°CBS, 24°CBU; lunghezza equivalente delle tubazioni: 5m"]
["","","","","","(2) - Riscaldamento: temp. interna 20°CBS; temp. esterna 7°CBS, 6°CBU; lunghezza equivalente del circuito frigorifero: 5m"]
["","","","","","(3) - Consultare i disegni separati per i dati elettrici"]