{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M / RXTM-N"]
[]
[]
[]
[]
["","","","","FTXTM30M2V1B / RXTM30N2V1B","FTXTM40M2V1B / RXTM40N2V1B"]
["Capacità di raffrescamento","Min.","","kW","0.70","0.70"]
["","Max.","","kW","4.50","5.10"]
["","Nom.","","kW","3.00","4.00"]
["Efficienza nominale","Consumo energetico annuale","","kWh","366","542"]
["","EER","","","4.10","3.71"]
["","COP","","","5.34","5.37"]
["","Classe energetica","Raffreddamento","","A","A"]
["","","Riscaldamento","","A","A"]
["Capacità di riscaldamento","Nom.","","kW","3.20","4.00"]
["","Min.","","kW","0.80","0.80"]
["","Max.","","kW","6.70","7.20"]
["Note","","","","(1) - Consultare i disegni separati per i dati elettrici","(1) - Consultare i disegni separati per i dati elettrici"]
["","","","","(2) - Raffrescamento: T2: temp. interna 26,6°CBS, 19,4°CBU, temp. esterna 48°CBS [Btu/hr/W]","(2) - Raffrescamento: T2: temp. interna 26,6°CBS, 19,4°CBU, temp. esterna 48°CBS [Btu/hr/W]"]
["","","","","(3) - Le capacità di riscaldamento nominali si riferiscono a: temperatura interna: 20°CBS, temperatura esterna: 7°CBS, 6°CBU, lunghezza equivalente delle tubazioni: 5m, dislivello: 0m.","(3) - Le capacità di riscaldamento nominali si riferiscono a: temperatura interna: 20°CBS, temperatura esterna: 7°CBS, 6°CBU, lunghezza equivalente delle tubazioni: 5m, dislivello: 0m."]