{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","43"]
["","","","Medio","dBA","35"]
["","","","Funzionamento silenzioso","dBA","21"]
["","","","Bassa","dBA","26"]
["","Raffrescamento","","Medio","dBA","35"]
["","","","Funzionamento silenzioso","dBA","21"]
["","","","Bassa","dBA","26"]
["","","","Alta","dBA","43"]
["Accessori standard","Manuale di installazione","","","","1"]
["","Manuale d’uso","","","","1"]
["","Telecomando ad infrarossi","","","","1"]
["","Batterie a secco AAA","","","","2"]
["","Supporto del telecomando","","","","1"]
["","Piastra di montaggio","","","","1"]
["","Filtro deodorizzante all'apatite di titanio","","","","2"]
["","Viti di fissaggio unità interna","","","","2"]
["Sistemi di comando","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35"]
["","Gas","","DE","mm","9.50"]
["","Scarico","","","","16 (diametro interno del tubo di collegamento)"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.030"]
["","Riscaldamento","","Nom.","kW","0.035"]
["Sound power level","Raffrescamento","","","dBA","58"]
["","Riscaldamento","","","dBA","58"]
["Dimensioni","Unità","","Larghezza","mm","770"]
["","","","Profondità","mm","225"]
["","","","Altezza","mm","285"]
["Rivestimento","Colore","","","","Bianco"]
["Peso","Unità","","","kg","9.0"]
["Power supply","Fase","","","","1~"]
["","Frequenza","","","Hz","50"]
["","Nome","","","","V1"]
["","Tensione","","","V","220-240"]
["Note","","","","","(1) - Consultare i disegni separati per i dati elettrici"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","0.03"]
["","Riscaldamento","","Nom.","kW","","0.035"]
["Rivestimento","Colore","","","","","Bianco"]
["Dimensioni","Unità","","Altezza","mm","","285"]
["","","","Larghezza","mm","","770"]
["","","","Profondità","mm","","225"]
["Peso","Unità","","","kg","","9"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","","11.4"]
["","","","Medio","m³/min","","8.2"]
["","","","Bassa","m³/min","","5.4"]
["","","","Funzionamento silenzioso","m³/min","","4.3"]
["","","Riscaldamento","Alta","m³/min","","10.8"]
["","","","Medio","m³/min","","7.8"]
["","","","Bassa","m³/min","","5.8"]
["","","","Funzionamento silenzioso","m³/min","","4.9"]
["Potenza sonora","Raffrescamento","","","dBA","","58"]
["","Riscaldamento","","","dBA","","58"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","43"]
["Pressione sonora","Raffrescamento","","Medio","dBA","","35"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","","26"]
["","","","Funzionamento silenzioso","dBA","","21"]
["","Riscaldamento","","Alta","dBA","","43"]
["Pressione sonora","Riscaldamento","","Medio","dBA","","35"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","","26"]
["","","","Funzionamento silenzioso","dBA","","21"]
["Attacchi tubazioni","Liquido","","DE","mm","","6.35"]
["","Gas","","DE","mm","","9.5"]
["","Scarico","","","","","16 (diametro interno del tubo di collegamento)"]
["Sistemi di comando","Infrared remote control","","","","","ARC480A11"]
["Sistemi di controllo","Telecomando con cavo","","","","","BRC944B2, BRC073A1"]
["Accessori standard","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Alimentazione","Nome","","","","","V1"]
["","Fase","","","","","1~"]
["","Frequenza","","","Hz","","50"]
["","Tensione","","","V","","220-240"]