{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-A"]
[]
[]
[]
[]
["","","","","","FVXTM30A3V1B"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.02"]
["","Riscaldamento","","Nom.","kW","0.03"]
["Rivestimento","Colore","","","","Bianco"]
["Dimensioni","Unità","","Altezza","mm","600"]
["","","","Larghezza","mm","750"]
["","","","Profondità","mm","238"]
["Peso","Unità","","","kg","17"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³;/min","9"]
["","","","Medio","m³;/min","6.7"]
["","","","Bassa","m³;/min","4.8"]
["","","","Funzionamento silenzioso","m³;/min","4"]
["","","Riscaldamento","Alta","m³;/min","9.4"]
["","","","Medio","m³;/min","6.8"]
["","","","Bassa","m³;/min","5.3"]
["","","","Funzionamento silenzioso","m³;/min","4"]
["Potenza sonora","Raffrescamento","","","dBA","53"]
["","Riscaldamento","","","dBA","53"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","39"]
["Pressione sonora","Raffrescamento","","Medio","dBA","32"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","25"]
["","","","Funzionamento silenzioso","dBA","20"]
["","Riscaldamento","","Alta","dBA","39"]
["Pressione sonora","Riscaldamento","","Medio","dBA","32"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","25"]
["","","","Funzionamento silenzioso","dBA","19"]
["Refrigerante","GWP","","","","675"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35"]
["","Gas","","DE","mm","9.5"]
["","Scarico","","","","VP20 (I.D. 20/O.D. 26)"]
["Sistemi di controllo","Infrared remote control","","","","ARC466A66"]
["Sistemi di controllo","Telecomando con cavo","","","","BRC073A1"]
["Accessori standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","2"]
["Alimentazione","Fase","","","","1~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","220-240"]