{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":102,"n_cols":12,"rows_kept":102,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMA-A"]
[]
[]
[]
[]
["","","","","","FXMA50A5VEB","FXMA63A5VEB","FXMA80A5VEB","FXMA100A5VEB","FXMA125A5VEB","FXMA200AXVMB","FXMA250AXVMB"]
["Livello pressione sonora","Riscaldamento","","Ad alta velocità del ventilatore","dBA","","","","","","48.0"]
["","","","A velocità del ventilatore bassa","dBA","","","","","","45.0"]
["","","","A velocità del ventilatore media","dBA","","","","","","46.5"]
["","Raffrescamento","","A velocità del ventilatore bassa","dBA","","","","","","45.0"]
["","","","Ad alta velocità del ventilatore","dBA","","","","","","48.0"]
["","","","A velocità del ventilatore media","dBA","","","","","","46.5"]
["Accessori standard","Manuale di installazione e uso","","","","","","","","","1"]
["","Materiale di fissaggio cavi","","","","","","","","","1"]
["","Rondella elastica","","","","","","","","","2"]
["","Vite a esagono","","","","","","","","","2"]
["","Rondella piana","","","","","","","","","8"]
["","Vite a esagono e rondella","","","","","","","","","49"]
["","Attacco tubazione del gas","","","","","","","","","1"]
["","Misure di sicurezza generali","","","","","","","","","1"]
["Refrigerante","GWP","","","","","","","","","675"]
["","Tipo","","","","","","","","","R-32"]
["Potenza assorbita - 50Hz","Raffrescamento","","Ad alta velocità del ventilatore","kW","","","","","","0.54"]
["","Riscaldamento","","Ad alta velocità del ventilatore","kW","","","","","","0.54"]
["Capacità di raffrescamento","Capacità totale","","Ad alta velocità del ventilatore","kW","","","","","","22.4"]
["","Nom.","","","kW","","","","","","22.4"]
["Piping connections","Liquido","","DE","mm","","","","","","9.5"]
["","","","Tipo","","","","","","","Attacco a cartella"]
["","Gas","","DE","mm","","","","","","19.1"]
["","","","Tipo","","","","","","","Flangia"]
["","Scarico","","","","","","","","","BSP1"]
["Livello potenza sonora","Raffrescamento","","Ad alta velocità del ventilatore","dBA","","","","","","75.0"]
["Dimensioni","Unità","","Larghezza","mm","","","","","","1,490"]
["","","","Profondità","mm","","","","","","1,100"]
["","","","Altezza","mm","","","","","","470"]
["Rivestimento","Materiale","","","","","","","","","Lamiera in acciaio zincato"]
["","Colour","","","","","","","","","Non verniciato"]
["Peso","Unità","","","kg","","","","","","105"]
["Ventilatore","Prevalenza - 50Hz","","Alta","Pa","","","","","","250"]
["","","","Bassa","Pa","","","","","","50"]
["","Prevalenza - 60Hz","","Alta","Pa","","","","","","250"]
["","","","Bassa","Pa","","","","","","50"]
["","Portata d'aria - 50Hz","Raffrescamento","Ad alta velocità del ventilatore","m³/min","","","","","","62"]
["","","","A velocità del ventilatore bassa","m³/min","","","","","","41"]
["Capacità di riscaldamento","Capacità totale","","Ad alta velocità del ventilatore","kW","","","","","","25.0"]
["","Nom.","","","kW","","","","","","25.0"]
["Corrente - 50Hz","Portata massima del fusibile (MFA)","","","A","","","","","","6"]
["Power supply","Fase","","","","","","","","","1~"]
["","Nome","","","","","","","","","VM"]
["","Frequenza","","","Hz","","","","","","50/60"]
["","Tensione","","","V","","","","","","220-240/220-230"]
["Capacità di raffrescamento","Capacità totale","","Ad alta velocità del ventilatore","kW","5.6","7.1","9.0","11.2","14.0","","28.0"]
["Capacità di riscaldamento","Capacità totale","","Ad alta velocità del ventilatore","kW","6.3","8.0","10.0","12.5","16.0","","31.5"]
["Potenza assorbita - 50Hz","Raffrescamento","","Ad alta velocità del ventilatore","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["","Riscaldamento","","Ad alta velocità del ventilatore","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["Dimensioni","Unità","","Altezza","mm","300","300","300","300","300","","470"]
["","","","Larghezza","mm","1,000","1,000","1,000","1,400","1,400","","1,490"]
["","","","Profondità","mm","700","700","700","700","700","","1,100"]
["Peso","Unità","","","kg","35","35","35","46","46","","115"]
["Rivestimento","Colore","","","","Non verniciato","Non verniciato","Non verniciato","Non verniciato","Non verniciato","","Non verniciato"]
["","Materiale","","","","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato","Lamiera in acciaio zincato","","Lamiera in acciaio zincato"]
["Altezza a soffitto richiesta >-=-mm","mm","","","","350","350","350","350","350"]
["Ventilatore","Portata d'aria - 50 Hz","Raffrescamento","Ad alta velocità del ventilatore","m³/min","18.0","19.5","25.0","32.0","36.0","","74"]
["","","","A velocità del ventilatore bassa","m³/min","15.0","16.0","20.0","23.0","26.0","","52"]
["","Prevalenza - 50Hz","","Alta","Pa","200","200","200","200","200","","250"]
["","Prevalenza - 60Hz","","Alta","Pa","200","200","200","200","200","","250"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","","R-32"]
["","GWP","","","","675","675","675","675","675","","675"]
["Livello di potenza sonora","Raffrescamento","","Ad alta velocità del ventilatore","dBA","61.0","64.0","67.0","65.0","70.0","","76.0"]
["Pressione sonora","Raffrescamento","","Ad alta velocità del ventilatore","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","A velocità del ventilatore media","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","Pressione sonora-=-Raffrescamento-=-A velocità del ventilatore bassa-=-dBA","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["","Riscaldamento","","Ad alta velocità del ventilatore","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","A velocità del ventilatore media","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","A velocità del ventilatore bassa","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["Attacchi tubazioni","Liquido","","Tipo","","Attacco a cartella","Attacco a cartella","Attacco a cartella","Attacco a cartella","Attacco a cartella","","Attacco a cartella"]
["","","","DE","mm","6.35","6.35","6.35","9.52","9.52","","9.5"]
["","Gas","","Tipo","","Attacco a cartella","Attacco a cartella","Attacco a cartella","Attacco a cartella","Attacco a cartella","","Flangia"]
["","","","DE","mm","12.7","12.7","12.7","15.9","15.9","","19.1"]
["","Scarico","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","","BSP1"]
["Filtro aria","Tipo","","","","Rete in resina","Rete in resina","Rete in resina","Rete in resina","Rete in resina"]
["Accessori standard","Washer for hanger bracket","","","","8","8","8","8","8"]
["","Drain hose","","","","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","","1"]
["","Insulation for fitting","","","","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1"]
["","Screws","","","","16","16","16","16","16"]
["","Sealing pad","","","","3","3","3","3","3"]
["Alimentazione","Nome","","","","VE","VE","VE","VE","VE","","VM"]
["","Fase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frequenza","","","Hz","50/60","50/60","50/60","50/60","50/60","","50/60"]
["","Tensione","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","","220-240/220-230"]
["Corrente - 50Hz","Portata massima del fusibile (MFA)","","","A","6","6","6","6","6","","6"]
["Ventilatore","Prevalenza - 50Hz","","Bassa","Pa","","","","","","","50"]
["","Prevalenza - 60Hz","","Bassa","Pa","","","","","","","50"]
["Accessori standard","General safety precautions","","","","","","","","","","1"]
["","Wire clamp material","","","","","","","","","","1"]
["","Spring washer","","","","","","","","","","2"]
["","Hexagon head screw","","","","","","","","","","2"]
["","Plain washer","","","","","","","","","","8"]
["","Hexagon head screw with washer","","","","","","","","","","49"]
["","Gas connection pipe","","","","","","","","","","1"]