{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","GCU-PXB1"]
[]
[]
[]
[]
["","","","","","GCU2020PXB1","GCU2040PXB1","GCU4070PXB1"]
["Capacità di refrigerazione","Temperatura media","","kW","kW","3.39","6.50","12.54"]
["Compressore","Numero di giri","","","giri/min","4,200","4,800","3,600"]
["Peso","Unità","","","kg","151","155","285"]
["Refrigerante","GWP","","","","1"]
["","Tipo","","","","R744 (CO2)"]
["Motore ventilatore","Potenza","","","W","115","115","230"]
["","Azionamento","","","","EC","EC","EC"]
["Scambiatore di calore","Tipo","","","","Standard rame/alluminio","Standard rame/alluminio","Standard rame/alluminio"]
["Potenza assorbita","Temperatura media","","Nom.","kW","1.81","3.81","7.99"]
["COP","Temperatura media","","Nom.","","1.87","1.70","1.57"]
["Dimensioni","Unità","","Larghezza","mm","574","574","773"]
["","","","Profondità","mm","1,452","1,452","1,684"]
["","","","Altezza","mm","799","799","1,438"]
["Motore ventilatore 2","Uscita","","","W","115","115","230"]
["Rivestimento","Colour","","","","Grigio chiaro RAL 7035","Grigio chiaro RAL 7035","Grigio chiaro RAL 7035"]
["Ventilatore","Type","","","","Assiale","Assiale","Assiale"]
["","Portata d'aria","Raffrescamento","Nom.","m³/min","63","63","126"]
["","Quantità","","","","1","1","2"]
["Power supply","Fase","","","","3~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","400"]