{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL1"]
[]
[]
[]
[]
["","","","","JEHCCU0135CL1"]
["Peso","Unità","","kg","61"]
["Dimensioni","Unità","Larghezza","mm","876"]
["","","Profondità","mm","430"]
["","","Altezza","mm","606"]
["Rivestimento","Colore","","","Grigio chiaro"]
["Ventilatore","Tipo","","","Assiale"]
["Power supply","Fase","","","1~"]
["","Frequenza","","Hz","50"]
["","Tensione","","V","230"]
["Note","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","(2) - Il livello della pressione sonora è misurato a 10m in camera anecoica"]
["","","","","(3) - Il suo funzionamento dipende dai gas fluorurati a effetto serra"]