{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","","47","48"]
["","Raffrescamento","","Alta","dBA","","46","48"]
["Accessori standard","Giunto (scarico)","","","","","1","1"]
["","Manuale di installazione","","","","","1","1"]
["Refrigerante","Charge","","","TCO2Eq","","2.2","2.2"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","1.05","1.05"]
["","Tipo","","","","","R-410A","R-410A"]
["Motore ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","","780","780"]
["","","Riscaldamento","Bassissimo","giri/min","","740","740"]
["Collegamenti tubazioni","Dislivello","int. - est.","Max.","m","","15","15"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","0,02 (per lunghezza delle tubazioni superiore ai 10m)","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["Compressore","Tipo","","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Dimensioni","Unità","","Larghezza","mm","","765","765"]
["","","","Profondità","mm","","285","285"]
["","","","Altezza","mm","","550","550"]
["Peso","Unità","","","kg","","35","35"]
["Ventilatore","Portata d'aria","Riscaldamento","Bassissimo","cfm","","932","932"]
["","","Raffrescamento","Bassissimo","cfm","","1,094","1,094"]
["Power supply","Fase","","","","","1~","1~"]
["","Frequenza","","","Hz","","50","50"]
["","Tensione","","","V","","220-240","220-240"]
["Note","","","","","(1) - 220V","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 230V","(3) - 230V","(3) - 240V"]
["","","","","","(4) - Campo di funzionamento in combinazione con Nexura, FVXG-K, raffrescamento: min. 10°CBS - max. 46°CBS; riscaldamento: min. -15°CBU - max. 18°CBU;","(4) - 240V","(4) - 240V","(4) - Campo di funzionamento in combinazione con Nexura, FVXG-K, raffrescamento: min. 10°CBS - max. 46°CBS; riscaldamento: min. -15°CBU - max. 18°CBU;"]
["","","","","","","(5) - Campo di funzionamento in combinazione con Nexura, FVXG-K, raffrescamento: min. 10°CBS - max. 46°CBS; riscaldamento: min. -15°CBU - max. 18°CBU;","(5) - Campo di funzionamento in combinazione con Nexura, FVXG-K, raffrescamento: min. 10°CBS - max. 46°CBS; riscaldamento: min. -15°CBU - max. 18°CBU;"]
["","","","","","","(6) - Contiene gas fluorurati a effetto serra","(6) - Contiene gas fluorurati a effetto serra"]
["Ventilatore","Portata d'aria","Raffrescamento","Bassissimo","m³/min","31.0","","","42.6"]
["","","Riscaldamento","Bassissimo","m³/min","26.4","","","38.3"]
["","","","Bassissimo","cfm","1094","","","1504"]
["","","Riscaldamento","Bassissimo","cfm","932","","","1352"]
["Dimensioni","Unità","","Altezza","mm","550","","","735"]
["","","","Larghezza","mm","765","","","825"]
["","","","Profondità","mm","285","","","300"]
["Peso","Unità","","","kg","35","","","48"]
["Motore del ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","780","","","670"]
["","","Riscaldamento","Bassissimo","giri/min","740","","","670"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","","","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10 (5)","","","-10 (5)"]
["","","","Max.","°CBS","46","","","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","-15","","","-15"]
["","","","Max.","°CBU","18","","","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","46","","","48"]
["","Riscaldamento","","Alta","dBA","47","","","48"]
["Refrigerante","Tipo","","","","R-410A","","","R-410A"]
["","Carica","","","kg","1.05","","","1.6"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","2.2","","","3.3"]
["","GWP","","","","2087.5","","","2087.5"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","20","","","30"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 10m)","","","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["","Dislivello","int. - est.","Max.","m","15","","","20"]
["Accessori standard","Installation manual","","","","1","","","1"]
["","Joint (drain)","","","","1","","","1"]
["Alimentazione","Fase","","","","1~","","","1~"]
["","Frequenza","","","Hz","50","","","50"]
["","Tensione","","","V","220-240","","","220-240"]