{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilatore","Portata d'aria","Raffrescamento","Bassissimo","m³/min","30.6","30.6"]
["","","Riscaldamento","Bassissimo","m³/min","27.2","27.2"]
["","","","Bassissimo","cfm","1080","1080"]
["","","Riscaldamento","Bassissimo","cfm","960","960"]
["Dimensioni","Unità","","Altezza","mm","550","550"]
["","","","Larghezza","mm","858","858"]
["","","","Profondità","mm","330","330"]
["Peso","Unità","","","kg","40","40"]
["Compressor","Type","","","","","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","46","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","-25","-25"]
["","","","Max.","°CBU","18","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","48","48"]
["","","","Bassa","dBA","44","44"]
["","Riscaldamento","","Alta","dBA","49","49"]
["","","","Bassa","dBA","45","45"]
["Refrigerante","Tipo","","","","R-410A","R-410A"]
["","Carica","","","kg","1","1"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","20","20"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 10m)","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["","Dislivello","int. - int.","Max.","m","15","15"]
["Accessori standard","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Alimentazione","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","220-240","220-240"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing"]