{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","49","","","52"]
["","","","Bassa","dBA","46","","","49"]
["","Raffrescamento","","Bassa","dBA","46","","","49"]
["","","","Alta","dBA","49","","","52"]
["Accessori standard","Attacco di scarico","","","","1","","","1"]
["","Manuale di installazione","","","","1","","","1"]
["Refrigerante","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Carica","","","kg","1.5","","","2.3"]
["","Tipo","","","","R-410A","","","R-410A"]
["Attacchi tubazioni","Dislivello","int. - est.","Max.","m","20","","","20"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 10m)","","","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","","","Compressore ermetico tipo Swing"]
["Dimensioni","Unità","","Larghezza","mm","825","","","900"]
["","","","Profondità","mm","300","","","320"]
["","","","Altezza","mm","735","","","770"]
["Peso","Unità","","","kg","48","","","71"]
["Power supply","Fase","","","","1~","","","1~"]
["","Frequenza","","","Hz","50","","","50"]
["","Tensione","","","V","220-240","","","220-240"]
["Note","","","","","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - 220V","","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria","(1) - 220V"]
["","","","","","(2) - Contiene gas fluorurati a effetto serra","(2) - 230V","","(2) - Contiene gas fluorurati a effetto serra","(2) - 230V"]
["Dimensioni","Unità","","Altezza","mm","","735","735","","770","770"]
["","","","Larghezza","mm","","825","825","","900","900"]
["","","","Profondità","mm","","300","300","","320","320"]
["Peso","Unità","","","kg","","48","48","","71","71"]
["Compressore","Tipo","","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","","-10","-10","","-10","-10"]
["","","","Max.","°CBS","","46","46","","46","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","","-15","-15","","-15","-15"]
["","","","Max.","°CBU","","18","20","","18","20"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","49","49","","52","52"]
["","","","Bassa","dBA","","46","46","","49","49"]
["","Riscaldamento","","Alta","dBA","","49","49","","52","52"]
["","","","Bassa","dBA","","46","46","","49","49"]
["Refrigerante","Tipo","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Carica","","","kg","","1.5","1.5","","2.3","2.3"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","30","30","","30","30"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","0,02 (per lunghezza delle tubazioni superiore ai 10m)","0,02 (per lunghezza delle tubazioni superiore ai 10m)","","0,02 (per lunghezza delle tubazioni superiore ai 10m)","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["","Dislivello","int. - est.","Max.","m","","20","20","","20","20"]
["Accessori standard","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Alimentazione","Fase","","","","","1~","1~","","1~","1~"]
["","Frequenza","","","Hz","","50","50","","50","50"]
["","Tensione","","","V","","220-240","220-240","","220-240","220-240"]
["Note","","","","","","(3) - 240V","","","(3) - 240V"]
["Accessori standard","Drain socket","","","","","","1","","","1"]
["Sound power level","Raffrescamento","","","dBA","","","","65"]