{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":11,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","47","47","48","48"]
["","Raffrescamento","","Alta","dBA","46","46","48","48"]
["Accessori standard","Tappo di scarico","","","","1","1","1","1"]
["","Manuale di installazione","","","","1","1","1","1"]
["","Etichetta relativa alla carica di refrigerante","","","","1","1","1"]
["","Etichette multilingue sui gas serra fluorurati","","","","1","1","Etichette multilingue sui gas serra fluorurati"]
["Refrigerante","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","1.0","1.20","1.3"]
["","Tipo","","","","R-410A","R-410A","R-410A","R-410A"]
["Motore del ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","780","780","780","790"]
["","","Riscaldamento","Bassissimo","giri/min","740","740","740","780"]
["Intervallo di funzionamento","Raffrescamento","T. esterna","Max.","°CBS","46","46","46","46"]
["","","","Min.","°CBS","-10","-10","-10","-10"]
["","Riscaldamento","T. esterna","Max.","°CBU","18","18","18","18"]
["","","","Min.","°CBU","-15","-15","-15","-15"]
["Attacchi tubazioni","Dislivello","int. - est.","Max.","m","","","15"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","","0,020 (per lunghezza delle tubazioni superiore ai 10m)"]
["Dimensioni","Unità","","Larghezza","mm","765","765","765","765"]
["","","","Profondità","mm","285","285","285","285"]
["","","","Altezza","mm","550","550","550","550"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Peso","Unità","","","kg","34","34","34","39"]
["Ventilatore","Portata d'aria","Riscaldamento","Bassissimo","cfm","904","904","904","960"]
["","","","Bassissimo","m³/min","25.6","25.6","25.6","27.2"]
["","","Raffrescamento","Bassissimo","m³/min","30.1","30.1","30.1","30.6"]
["","","","Bassissimo","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Contiene gas fluorurati a effetto serra","(4) - Contiene gas fluorurati a effetto serra","(4) - Contiene gas fluorurati a effetto serra","(4) - Contiene gas fluorurati a effetto serra"]
["Ventilatore","Portata d'aria","Raffrescamento","Bassissimo","m³/min","","","","","48.9","45.0"]
["","","Riscaldamento","Bassissimo","m³/min","","","","","43.1","46.3"]
["","","","Bassissimo","cfm","","","","","1727","1589"]
["","","Riscaldamento","Bassissimo","cfm","","","","","1522","1635"]
["Dimensioni","Unità","","Altezza","mm","","","","","735","735"]
["","","","Larghezza","mm","","","","","825","825"]
["","","","Profondità","mm","","","","","300","300"]
["Peso","Unità","","","kg","","","","","47","48"]
["Motore del ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","","","","","670"]
["","","Riscaldamento","Bassissimo","giri/min","","","","","670"]
["Compressore","Tipo","","","","","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","","","","","-10","-10"]
["","","","Max.","°CBS","","","","","46","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","","","","","-15","-15"]
["","","","Max.","°CBU","","","","","18","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","","","","48","49"]
["","","","Bassa","dBA","","","","","44","46"]
["","Riscaldamento","","Alta","dBA","","","","","48","49"]
["","","","Bassa","dBA","","","","","45","46"]
["Refrigerante","Tipo","","","","","","","","R-410A","R-410A"]
["","Carica","","","kg","","","","","1.7","1.5"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","","","","30","30"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","","","","0,020 (per lunghezza delle tubazioni superiore ai 10m)","0,020 (per lunghezza delle tubazioni superiore ai 10m)"]
["","Dislivello","int. - est.","Max.","m","","","","","20.0","20"]
["Accessori standard","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Alimentazione","Fase","","","","","","","","1~","1~"]
["","Frequenza","","","Hz","","","","","50","50"]
["","Tensione","","","V","","","","","220-230-240","220-230-240"]
["Note","","","","","","","","","","(1) - 230V"]