{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B9","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Dimensioni","Unità","","Altezza","mm","693"]
["","","","Larghezza","mm","795"]
["","","","Profondità","mm","300"]
["Peso","Unità","","","kg","50"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10"]
["","","","Max.","°CBS","43"]
["","Riscaldamento","T. esterna","Min.","°CBU","-20"]
["","","","Max.","°CBU","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","46"]
["","Riscaldamento","","Alta","dBA","46"]
["Refrigerante","Tipo","","","","R-32"]
["","Carica","","","kg","1.34"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","0.9"]
["","GWP","","","","675"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","10"]
["","Dislivello","int. - est.","Max.","m","8"]
["Accessori standard","Installation manual","","","","1"]
["","Operation manual","","","","1"]
["Alimentazione","Fase","","","","1~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Dimensioni","Unità","","Altezza","mm","","693","693","693"]
["","","","Larghezza","mm","","795","795","795"]
["","","","Profondità","mm","","300","300","300"]
["Peso","Unità","","","kg","","50","50","50"]
["Compressore","Type","","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Operation range","Raffresc.","T. esterna","Min.","°CBS","","-10","-10","-10"]
["","","","Max.","°CBS","","43","43","43"]
["","Riscaldamento","T. esterna","Min.","°CBU","","-20","-20","-20"]
["","","","Max.","°CBU","","18","18","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","48","49","49"]
["","Riscaldamento","","Alta","dBA","","48","50","50"]
["Refrigerante","Tipo","","","","","R-32","R-32","R-32"]
["","Carica","","","kg","","1.34","1.34","1.34"]
["","GWP","","","","","675","675","675"]
["Attacchi tubazioni","Dislivello","int. - est.","Max.","m","","8","8","8"]
["Accessori standard","Manuale d’uso","","","","","1","1","1"]
["","Manuale di installazione","","","","","1","1","1"]
["Power supply","Fase","","","","","1~","1~","1~"]
["","Frequenza","","","Hz","","50","50","50"]
["","Tensione","","","V","","220-240","220-240","220-240"]
["Note","","","","","","(4) - Contiene gas fluorurati a effetto serra","(4) - Contiene gas fluorurati a effetto serra","(4) - Contiene gas fluorurati a effetto serra"]