{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQG-LV1L"]
[]
[]
[]
[]
["","","","","","RZQG71L9V1L"]
["Potenza sonora","Raffrescamento","","","dBA","64"]
["Dimensioni","Unità","","Altezza","mm","990"]
["","","","Larghezza","mm","940"]
["","","","Profondità","mm","320"]
["Peso","Unità","","","kg","69.0"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-15"]
["","","","Max.","°CBS","50"]
["","Riscaldamento","T. esterna","Min.","°CBU","-20"]
["","","","Max.","°CBU","16"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","48"]
["","Riscaldamento","","Nom.","dBA","50"]
["","Modalità notturna","","Livello 1","dBA","43"]
["Refrigerante","Carica","","","kg","2.9"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","6.10"]
["","GWP","","","","2087.5"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","50"]
["","Dislivello","int. - est.","Max.","m","30.0"]
["","","int. - int.","Max.","m","0.5"]
["Accessori standard","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Alimentazione","Frequenza","","","Hz","50"]
["Note","","","","","(1) - 3 con ricarica"]