{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLCO2"]
[]
[]
[]
[]
["","","","","WLCO2."]
["Massimo numero di unità interne collegabili","","","","0"]
["Massimo numero di unità esterne collegabili @","","","","0"]
["Rivestimento","Colore","","","Bianco"]
["","Coperchio pulsantiera","","","No"]
["","LED di funzionamento","Colore","","Verde"]
["Dimensioni","Unità","Altezza","mm","95"]
["","","Larghezza","mm","95.0"]
["","","Profondità","mm","62.0"]
["","Unità imballata","Altezza","mm","565"]
["","","Larghezza","mm","375"]
["","","Profondità","mm","280"]
["Peso","Unità","","kg","0.126"]
["Imballaggio","Materiale","","","Cartone"]
["Guarnizione","Peso","","kg","0.046"]
["Temperatura esterna","Funzionamento","Min.","°C","-10"]
["","","Max.","°C","50"]
["","Magazzinamento","Min.","°C","-20"]
["","","Max.","°C","60"]
["","Temperatura esterna-=-Umidità relativa <-=-%","","%","90"]
["Installazione","","","","Installazione in spazi interni"]