{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSXB14A"]
[]
[]
[]
[]
["","","","","","EPSXB14P30AF","EPSXB14P50AF"]
["Gehäuse","Farbe","","","","Verkehrsweiß (RAL9016), Graphitschwarz (RAL9011), Tiefschwarz (RAL9005)","Verkehrsweiß (RAL9016), Graphitschwarz (RAL9011), Tiefschwarz (RAL9005)"]
["","Material","","","","Schlagfestes Polypropylen","Schlagfestes Polypropylen"]
["Abmessungen","Maßeinheit","","Höhe","mm","1914","1906"]
["","","","Breite","mm","590","785"]
["","","","Tiefe","mm","671","837"]
["Gewicht","Maßeinheit","","","kg","87.0","109"]
["PED","Kategorie","","","","Art 4.3","Art 4.3"]
["Schallleistungspegel","Nom.","","","dB(A)","49.0","49.0"]
["Schalldruckpegel","Schalldruckpegel-=-Nom.-=-dBA","","","dB(A)","35.0","35.0"]
["Betriebsbereich","Heizen","Wasserseite","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["","Kühlung","Umgebung","Min.","°CTK","0 (3)","0 (3)"]
["","","Wasserseite","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","230","230"]
["Elektroheizung","Spannungsversorgung","","Bezeichnung","","6V / 9W","6V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~"]
["","","","Frequenz","Hz","50","50"]
["","","","Spannung","V","230/400","230/400"]
["","Empfohlene Sicherungen","","","A","0 (4)","0 (4)"]
["Hinweise","","","","","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897"]
["","","","","","(2) - Erforderliches Mindestvolumen, ohne Volumen im Gerät","(2) - Erforderliches Mindestvolumen, ohne Volumen im Gerät"]
["","","","","","(3) - Siehe Zeichnung „Betriebsgrenzen“","(3) - Siehe Zeichnung „Betriebsgrenzen“"]
["","","","","","(4) - Siehe Elektroschaltplan und Installationshandbuch für Angaben zu korrekten, empfohlenen Sicherungen je nach Stromversorgung und Netzanschluss","(4) - Siehe Elektroschaltplan und Installationshandbuch für Angaben zu korrekten, empfohlenen Sicherungen je nach Stromversorgung und Netzanschluss"]